This is mpfr.info, produced by makeinfo version 4.2 from mpfr.texi.

START-INFO-DIR-ENTRY
* mpfr: (mpfr.info).               Multiple Precision Floating-Point Reliable Library.
END-INFO-DIR-ENTRY

   This file documents MPFR, a library for reliable multiple precision
floating-point arithmetic

   Copyright (C) 1999-2002, Free Software Foundation.

   Permission is granted to make and distribute verbatim copies of this
manual provided the copyright notice and this permission notice are
preserved on all copies.

   Permission is granted to copy and distribute modified versions of
this manual under the conditions for verbatim copying, provided that
the entire resulting derived work is distributed under the terms of a
permission notice identical to this one.

   Permission is granted to copy and distribute translations of this
manual into another language, under the above conditions for modified
versions, except that this permission notice may be stated in a
translation approved by the Foundation.


File: mpfr.info,  Node: Top,  Next: Copying,  Prev: (dir),  Up: (dir)

MPFR
****

   This manual documents how to install and use the Multiple Precision
Floating-Point Reliable Library, version 2.0.1

* Menu:

* Copying::                   GMP Copying Conditions (LGPL).
* Introduction to MPFR::      Brief introduction to MPFR.
* Installing MPFR::           How to configure and compile the MPFR library.
* MPFR Basics::               What every MPFR user should now.
* Reporting Bugs::            How to usefully report bugs.
* Floating-point Functions::  Functions for arithmetic on floats.

* Contributors::
* References::
* Concept Index::
* Function Index::


File: mpfr.info,  Node: Copying,  Next: Introduction to MPFR,  Prev: Top,  Up: Top

MPFR Copying Conditions
***********************

   This library is "free"; this means that everyone is free to use it
and free to redistribute it on a free basis.  The library is not in the
public domain; it is copyrighted and there are restrictions on its
distribution, but these restrictions are designed to permit everything
that a good cooperating citizen would want to do.  What is not allowed
is to try to prevent others from further sharing any version of this
library that they might get from you.

   Specifically, we want to make sure that you have the right to give
away copies of the library, that you receive source code or else can
get it if you want it, that you can change this library or use pieces
of it in new free programs, and that you know you can do these things.

   To make sure that everyone has such rights, we have to forbid you to
deprive anyone else of these rights.  For example, if you distribute
copies of the MPFR library, you must give the recipients all the rights
that you have.  You must make sure that they, too, receive or can get
the source code.  And you must tell them their rights.

   Also, for our own protection, we must make certain that everyone
finds out that there is no warranty for the MPFR library.  If it is
modified by someone else and passed on, we want their recipients to
know that what they have is not what we distributed, so that any
problems introduced by others will not reflect on our reputation.

   The precise conditions of the license for the MPFR library are found
in the Lesser General Public License that accompanies the source code.
See the file COPYING.LIB.


File: mpfr.info,  Node: Introduction to MPFR,  Next: Installing MPFR,  Prev: Copying,  Up: Top

Introduction to MPFR
********************

   MPFR is a portable library written in C for arbitrary precision
arithmetic on reliable floating-point numbers. It is based on the GNU
MP library.  It aims to extend the class of floating-point numbers
provided by the GNU MP library by "reliable" floating-point numbers. It
may replace the GNU MP floating-point numbers in a future release. The
main differences with the `mpf' class are:

   * the `mpfr' code is portable, i.e. the result of any operation does
     not depend (or should not) on the machine word size
     `mp_bits_per_limb' (32 or 64 on most machines);

   * the precision in bits can be set exactly to any valid value for
     each variable (including very small precision);

   * `mpfr' provides the four rounding modes from the IEEE 754 standard.

   In particular, with a precision of 53 bits, `mpfr' should be able to
exactly reproduce all computations with double-precision machine
floating-point numbers (`double' type in C), except the default
exponent range is much wider and subnormal numbers are not implemented.

   This version of MPFR is released under the GNU Lesser General Public
License.  It is permitted to link MPFR to non-free programs, as long as
when distributing them the MPFR source code and a means to re-link with
a modified MPFR is provided.

How to use this Manual
======================

   Everyone should read *Note MPFR Basics::.  If you need to install
the library yourself, you need to read *Note Installing MPFR::, too.

   The rest of the manual can be used for later reference, although it
is probably a good idea to glance through it.


File: mpfr.info,  Node: Installing MPFR,  Next: Reporting Bugs,  Prev: Introduction to MPFR,  Up: Top

Installing MPFR
***************

   To build MPFR, you first have to install GNU MP (version 4.0.1 or
higher) on your computer.  You need a C compiler, preferably GCC, but
any reasonable compiler should work.  And you need a standard Unix
`make' program, plus some other standard Unix utility programs.

   Here are the steps needed to install the library on Unix systems
(more details are provided in the `INSTALL' file):

  1. In most cases, `./configure --with-gmp=/usr/local/gmp' should work,
     where the directory `/usr/local/gmp' is where you have installed
     GNU MP.  When you install GNU MP, you have to copy the files
     `config.h', `gmp-impl.h', `gmp-mparam.h' and `longlong.h' from the
     GNU MP source directory to `/usr/local/gmp/include'; these
     additional files are needed by MPFR.  If you get error messages,
     you might check that you use the same compiler and compile options
     as for GNU MP (see the `INSTALL' file).

  2. `make'

     This will compile MPFR, and create a library archive file
     `libmpfr.a' in the working directory.

  3. `make check'

     This will make sure MPFR was built correctly.  If you get error
     messages, please report this to `mpfr@loria.fr'.  (*Note Reporting
     Bugs::, for information on what to include in useful bug reports.)

  4. `make install'

     This will copy the files `mpfr.h' and `mpf2mpfr.h', and
     `libmpfr.a', to the directories `/usr/local/include' and
     `/usr/local/lib' respectively (or if you passed the `--prefix'
     option to `configure', to the directory given as argument to
     `--prefix').  This will also install `mpfr.info' in
     `/usr/local/info'.

   There are some other useful make targets:

   * `mpfr.dvi' or `dvi'

     Create a DVI version of the manual, in `mpfr.dvi'.

   * `mpfr.ps'

     Create a Postscript version of the manual, in `mpfr.ps'.

   * `clean'

     Delete all object files and archive files, but not the
     configuration files.

   * `distclean'

     Delete all files not included in the distribution.

   * `uninstall' Delete all files copied by `make install'.

Known Build Problems
====================

   MPFR suffers from all bugs from the GNU MP library, plus many many
more.

   Please report other problems to `mpfr@loria.fr'.  *Note Reporting
Bugs::.  Some bug fixes are available on the MPFR web page
`http://www.loria.fr/projets/mpfr/' or `http://www.mpfr.org/'.


File: mpfr.info,  Node: Reporting Bugs,  Next: MPFR Basics,  Prev: Installing MPFR,  Up: Top

Reporting Bugs
**************

   If you think you have found a bug in the MPFR library, first have a
look on the MPFR web page `http://www.loria.fr/projets/mpfr/' or
`http://www.mpfr.org/': perhaps this bug is already known, in which
case you will find a workaround for it.  Otherwise, please investigate
and report it. We have made this library available to you, and it is
not to ask too much from you, to ask you to report the bugs that you
find.

   There are a few things you should think about when you put your bug
report together.

   You have to send us a test case that makes it possible for us to
reproduce the bug.  Include instructions on how to run the test case.

   You also have to explain what is wrong; if you get a crash, or if
the results printed are incorrect and in that case, in what way.

   Please include compiler version information in your bug report.
This can be extracted using `cc -V' on some machines, or, if you're
using gcc, `gcc -v'.  Also, include the output from `uname -a'.

   If your bug report is good, we will do our best to help you to get a
corrected version of the library; if the bug report is poor, we won't
do anything about it (aside of chiding you to send better bug reports).

   Send your bug report to: `mpfr@loria.fr'.

   If you think something in this manual is unclear, or downright
incorrect, or if the language needs to be improved, please send a note
to the same address.


File: mpfr.info,  Node: MPFR Basics,  Next: Floating-point Functions,  Prev: Reporting Bugs,  Up: Top

MPFR Basics
***********

   All declarations needed to use MPFR are collected in the include file
`mpfr.h'.  It is designed to work with both C and C++ compilers.  You
should include that file in any program using the MPFR library:

   `#include "mpfr.h"'

Nomenclature and Types
======================

"Floating-point number" or "Float" for short, is an arbitrary precision
mantissa with a limited precision exponent.  The C data type for such
objects is `mpfr_t'.  A floating-point number can have three special
values: Not-a-Number (NaN) or plus or minus Infinity. NaN represents a
value which cannot be represented in the floating-point format, like 0
divided by 0, or Infinity minus Infinity.

The "Precision" is the number of bits used to represent the mantissa of
a floating-point number; the corresponding C data type is `mp_prec_t'.
The precision can be any integer between `MPFR_PREC_MIN' and
`MPFR_PREC_MAX'. In the current implementation, `MPFR_PREC_MIN' is
equal to 2 and `MPFR_PREC_MAX' is equal to `ULONG_MAX'.

The "rounding mode" specifies the way to round the result of a
floating-point operation, in case the exact result can not be
represented exactly in the destination mantissa; the corresponding C
data type is `mp_rnd_t'.

A "limb" means the part of a multi-precision number that fits in a
single word.  (We chose this word because a limb of the human body is
analogous to a digit, only larger, and containing several digits.)
Normally a limb contains 32 or 64 bits.  The C data type for a limb is
`mp_limb_t'.

Function Classes
================

   There is only one class of functions in the MPFR library:

  1. Functions for floating-point arithmetic, with names beginning with
     `mpfr_'.  The associated type is `mpfr_t'.

MPFR Variable Conventions
=========================

   As a general rule, all MPFR functions expect output arguments before
input arguments.  This notation is based on an analogy with the
assignment operator.

   MPFR allows you to use the same variable for both input and output
in the same expression.  For example, the main function for
floating-point multiplication, `mpfr_mul', can be used like this:
`mpfr_mul (x, x, x, rnd_mode)'.  This computes the square of X with
rounding mode `rnd_mode' and puts the result back in X.

   Before you can assign to an MPFR variable, you need to initialize it
by calling one of the special initialization functions.  When you're
done with a variable, you need to clear it out, using one of the
functions for that purpose.

   A variable should only be initialized once, or at least cleared out
between each initialization.  After a variable has been initialized, it
may be assigned to any number of times.

   For efficiency reasons, avoid to initialize and clear out a variable
in loops.  Instead, initialize it before entering the loop, and clear
it out after the loop has exited.

   You don't need to be concerned about allocating additional space for
MPFR variables, since any variable has a mantissa of fixed size.  Hence
unless you change its precision, or clear and reinitialize it, a
floating-point variable will have the same allocated space during all
its life.

Compatibility with MPF
======================

   A header file `mpf2mpfr.h' is included in the distribution of MPFR
for compatibility with the GNU MP class MPF.  After inserting the
following two lines after the `#include "gmp.h"' line,

   `#include "mpfr.h"'

   `#include "mpf2mpfr.h"'

   any program written for MPF can be linked directly with MPFR without
any changes.  All operations are then performed with the default MPFR
rounding mode, which can be reset with `mpfr_set_default_rounding_mode'.

 - Global Variable: mp_rnd_t __gmp_default_rounding_mode
     The default rounding mode (to nearest initially).

Getting the Latest Version of MPFR
==================================

   The latest version of MPFR is available from
`http://www.loria.fr/projets/mpfr/' or `http://www.mpfr.org/'.


File: mpfr.info,  Node: Floating-point Functions,  Next: Contributors,  Prev: MPFR Basics,  Up: Top

Floating-point Functions
************************

   The floating-point functions expect arguments of type `mpfr_t'.

   The MPFR floating-point functions have an interface that is similar
to the GNU MP integer functions.  The function prefix for
floating-point operations is `mpfr_'.

   There is one significant characteristic of floating-point numbers
that has motivated a difference between this function class and other
MPFR function classes: the inherent inexactness of floating-point
arithmetic.  The user has to specify the precision of each variable.  A
computation that assigns a variable will take place with the precision
of the assigned variable; the cost of that computation should not
depend from the precision of variables used as input on average.

   The precision of a calculation is defined as follows: Compute the
requested operation exactly (with "infinite precision"), and round the
result to the destination variable precision with the given rounding
mode.  Even if the user has asked for a very high precision, MP will
not calculate with superfluous digits.  For example, if two
low-precision numbers of nearly equal magnitude are added, the
precision of the result will be limited to what is required to
represent the result accurately.

   The MPFR floating-point functions are intended to be a smooth
extension of the IEEE P754 arithmetic. The results obtained on one
computer should not differ from the results obtained on a computer with
a different word size.

* Menu:

* Rounding Modes::
* Exceptions::
* Initializing Floats::
* Assigning Floats::
* Simultaneous Float Init & Assign::
* Converting Floats::
* Float Arithmetic::
* Float Comparison::
* I/O of Floats::
* Miscellaneous Float Functions::


File: mpfr.info,  Node: Rounding Modes,  Next: Exceptions,  Prev: Floating-point Functions,  Up: Floating-point Functions

Rounding Modes
==============

   The following four rounding modes are supported:
   * `GMP_RNDN': round to nearest

   * `GMP_RNDZ': round towards zero

   * `GMP_RNDU': round towards plus infinity

   * `GMP_RNDD': round towards minus infinity
   The `round to nearest' mode works as in the IEEE P754 standard: in
case the number to be rounded lies exactly in the middle of two
representable numbers, it is rounded to the one with the least
significant bit set to zero.  For example, the number 5, which is
represented by (101) in binary, is rounded to (100)=4 with a precision
of two bits, and not to (110)=6.  This rule avoids the "drift"
phenomenon mentioned by Knuth in volume 2 of The Art of Computer
Programming (section 4.2.2, pages 221-222).

   Most MPFR functions take as first argument the destination variable,
as second and following arguments the input variables, as last argument
a rounding mode, and have a return value of type `int'. If this value
is zero, it means that the value stored in the destination variable is
the exact result of the corresponding mathematical function. If the
returned value is positive (resp. negative), it means the value stored
in the destination variable is greater (resp. lower) than the exact
result.  For example with the `GMP_RNDU' rounding mode, the returned
value is usually positive, except when the result is exact, in which
case it is zero.  In the case of an infinite result, it is considered
as inexact when it was obtained by overflow, and exact otherwise.  A
NaN result (Not-a-Number) always corresponds to an inexact return value.

 - Function: void mpfr_set_default_rounding_mode (mp_rnd_t RND)
     Sets the default rounding mode to RND.  The default rounding mode
     is to nearest initially.

 - Function: int mpfr_round_prec (mpfr_t X, mp_rnd_t RND, mp_prec_t
          PREC)
     Rounds X according to RND with precision PREC, which may be
     different from that of X.  If PREC is greater or equal to the
     precision of X, then new space is allocated for the mantissa, and
     it is filled with zeroes.  Otherwise, the mantissa is rounded to
     precision PREC with the given direction. In both cases, the
     precision of X is changed to PREC.  The returned value is zero
     when the result is exact, positive when it is greater than the
     original value of X, and negative when it is smaller.  The
     precision PREC can be any integer between `MPFR_PREC_MIN' and
     `MPFR_PREC_MAX'.

 - Function: void mpfr_set_machine_rnd_mode (mp_rnd_t RND)
     Set the machine rounding mode to RND.  This function is provided
     only when the operating system supports the ISOC9X standard
     interface for setting rounding modes (i.e. through the header file
     <fenv.h>).

 - Function: char * mpfr_print_rnd_mode (mp_rnd_t RND)
     Returns the input string (GMP_RNDD, GMP_RNDU, GMP_RNDN, GMP_RNDZ)
     corresponding to the rounding mode RND or a null pointer if RND is
     an invalid rounding mode.


File: mpfr.info,  Node: Exceptions,  Next: Initializing Floats,  Prev: Rounding Modes,  Up: Floating-point Functions

Exceptions
==========

   Note: Overflow handling is still experimental and currently
implemented very partially. If an overflow occurs internally at the
wrong place, anything can happen (crash, wrong results, etc).

 - Function: mp_exp_t mpfr_get_emin (void)
 - Function: mp_exp_t mpfr_get_emax (void)
     Return the (current) smallest and largest exponents allowed for a
     floating-point variable.

 - Function: int mpfr_set_emin (mp_exp_t EXP)
 - Function: int mpfr_set_emax (mp_exp_t EXP)
     Set the smallest and largest exponents allowed for a
     floating-point variable.  Return a non-zero value when EXP is not
     in the range accepted by the implementation (in that case the
     smallest or largest exponent is not changed), and zero otherwise.
     If the user changes the exponent range, it is her/his
     responsibility to check that all current floating-point variables
     are in the new allowed range (for example using `mpfr_check_range',
     otherwise the subsequent behaviour will be undefined, in the sense
     of the ISO C standard.

 - Function: int mpfr_check_range (mpfr_t X, mp_rnd_t RND)
     Return zero if the exponent of X is in the current allowed range
     (see `mpfr_get_emin' and `mpfr_get_emax'), otherwise reset X
     according to the current floating-point system and the rounding
     mode RND, and return a positive value if the rounded result is
     larger than the original one, a negative value otherwise (the
     result cannot be exact in that case).

 - Function: void mpfr_clear_underflow (void)
 - Function: void mpfr_clear_overflow (void)
 - Function: void mpfr_clear_nanflag (void)
 - Function: void mpfr_clear_inexflag (void)
     Clear the underflow, overflow, invalid, and inexact flags.

 - Function: void mpfr_clear_flags (void)
     Clear all global flags (underflow, overflow, inexact, invalid).

 - Function: int mpfr_underflow_p (void)
 - Function: int mpfr_overflow_p (void)
 - Function: int mpfr_nanflag_p (void)
 - Function: int mpfr_inexflag_p (void)
     Return the corresponding (underflow, overflow, invalid, inexact)
     flag, which is non-zero iff the flag is set.


File: mpfr.info,  Node: Initializing Floats,  Next: Assigning Floats,  Prev: Exceptions,  Up: Floating-point Functions

Initialization and Assignment Functions
=======================================

 - Function: void mpfr_set_default_prec (mp_prec_t PREC)
     Set the default precision to be *exactly* PREC bits.  The
     precision of a variable means the number of bits used to store its
     mantissa.  All subsequent calls to `mpfr_init' will use this
     precision, but previously initialized variables are unaffected.
     This default precision is set to 53 bits initially.  The precision
     can be any integer between `MPFR_PREC_MIN' and `MPFR_PREC_MAX'.

 - Function: mp_prec_t mpfr_get_default_prec ()
     Returns the default MPFR precision in bits.

   An `mpfr_t' object must be initialized before storing the first
value in it.  The functions `mpfr_init' and `mpfr_init2' are used for
that purpose.

 - Function: void mpfr_init (mpfr_t X)
     Initialize X, and set its value to NaN.  Normally, a variable
     should be initialized once only or at least be cleared, using
     `mpfr_clear', between initializations.  The precision of X is the
     default precision, which can be changed by a call to
     `mpfr_set_default_prec'.

 - Function: void mpfr_init2 (mpfr_t X, mp_prec_t PREC)
     Initialize X, set its precision to be *exactly* PREC bits, and set
     its value to NaN.  Normally, a variable should be initialized once
     only or at least be cleared, using `mpfr_clear', between
     initializations.  To change the precision of a variable which has
     already been initialized, use `mpfr_set_prec' instead.  The
     precision PREC can be any integer between `MPFR_PREC_MIN' and
     `MPFR_PREC_MAX'.

 - Function: void mpfr_clear (mpfr_t X)
     Free the space occupied by X.  Make sure to call this function for
     all `mpfr_t' variables when you are done with them.

   Here is an example on how to initialize floating-point variables:
     {
       mpfr_t x, y;
       mpfr_init (x);			/* use default precision */
       mpfr_init2 (y, 256);		/* precision _exactly_ 256 bits */
       ...
       /* Unless the program is about to exit, do ... */
       mpfr_clear (x);
       mpfr_clear (y);
     }

   The following two functions are useful for changing the precision
during a calculation.  A typical use would be for adjusting the
precision gradually in iterative algorithms like Newton-Raphson, making
the computation precision closely match the actual accurate part of the
numbers.

 - Function: int mpfr_set_prec (mpfr_t X, mp_prec_t PREC)
     Reset the precision of X to be *exactly* PREC bits.  The previous
     value stored in X is lost. It is equivalent to a call to
     `mpfr_clear(x)' followed by a call to `mpfr_init2(x, prec)', but
     more efficient as no allocation is done in case the current
     allocated space for the mantissa of X is enough.  The precision
     PREC can be any integer between `MPFR_PREC_MIN' and
     `MPFR_PREC_MAX'.  It returns a non-zero value iff the memory
     allocation failed.

     In case you want to keep the previous value stored in X, use
     `mpfr_round_prec' instead.

 - Function: mp_prec_t mpfr_get_prec (mpfr_t X)
     Return the precision actually used for assignments of X, i.e.  the
     number of bits used to store its mantissa.

 - Function: void mpfr_set_prec_raw (mpfr_t X, unsigned long int P)
     Reset the precision of X to be *exactly* PREC bits.  The only
     difference with `mpfr_set_prec' is that P is assumed to be small
     enough so that the mantissa fits into the current allocated memory
     space for X. Otherwise an error will occur.


File: mpfr.info,  Node: Assigning Floats,  Next: Simultaneous Float Init & Assign,  Prev: Initializing Floats,  Up: Floating-point Functions

Assignment Functions
====================

   These functions assign new values to already initialized floats
(*note Initializing Floats::).

 - Function: int mpfr_set (mpfr_t ROP, mpfr_t OP, mp_rnd_t RND)
 - Function: int mpfr_set_ui (mpfr_t ROP, unsigned long int OP,
          mp_rnd_t RND)
 - Function: int mpfr_set_si (mpfr_t ROP, long int OP, mp_rnd_t RND
 - Function: int mpfr_set_d (mpfr_t ROP, double OP, mp_rnd_t RND)
 - Function: int mpfr_set_z (mpfr_t ROP, mpz_t OP, mp_rnd_t RND)
 - Function: int mpfr_set_q (mpfr_t ROP, mpq_t OP, mp_rnd_t RND)
     Set the value of ROP from OP, rounded to the precision of ROP
     towards the given direction RND.  Please note that even a `long
     int' may have to be rounded, if the destination precision is less
     than the machine word width.  The return value is zero when
     ROP=OP, positive when ROP>OP, and negative when ROP<OP.  For
     `mpfr_set_d', be careful that the input number OP may not be
     exactly representable as a double-precision number (this happens
     for 0.1 for instance), in which case it is first rounded by the C
     compiler to a double-precision number, and then only to a mpfr
     floating-point number.

 - Function: int mpfr_set_str (mpfr_t X, char *S, int BASE, mp_rnd_t
          RND)
     Set X to the value of the string S in base BASE (between 2 and
     36), rounded in direction RND to the precision of X.  The exponent
     is read in decimal.  This function returns -1 if an internal
     overflow occurred (for instance, because the exponent is too
     large). Otherwise it returns 0 if the base is valid and if the
     entire string up to the final '\0' is a valid number in base BASE,
     and 1 if the input is incorrect.

 - Function: void mpfr_set_str_raw (mpfr_t X, char *S)
     Set X to the value of the binary number in string S, which has to
     be of the form +/-xxxx.xxxxxxEyy. The exponent is read in decimal,
     but is interpreted as the power of two to be multiplied by the
     mantissa.  The mantissa length of S has to be less or equal to the
     precision of X, otherwise an error occurs.  If S starts with `N',
     it is interpreted as NaN (Not-a-Number); if it starts with `I'
     after the sign, it is interpreted as infinity, with the
     corresponding sign.

 - Function: int mpfr_set_f (mpfr_t X, mpf_t Y, mp_rnd_t RND)
     Set X to the GNU MP floating-point number Y, rounded with the RND
     mode and the precision of X.  The returned value is zero when X=Y,
     positive when X>Y, and negative when X<Y.

 - Function: void mpfr_set_inf (mpfr_t X, int SIGN)
 - Function: void mpfr_set_nan (mpfr_t X)
     Set the variable X to infinity or NaN (Not-a-Number) respectively.
     In `mpfr_set_inf', X is set to plus infinity iff SIGN is positive.

 - Function: void mpfr_swap (mpfr_t X, mpfr_t Y)
     Swap the values X and Y efficiently. Warning: the precisions are
     exchanged too; in case the precisions are different, `mpfr_swap'
     is thus not equivalent to three `mpfr_set' calls using a third
     auxiliary variable.


File: mpfr.info,  Node: Simultaneous Float Init & Assign,  Next: Converting Floats,  Prev: Assigning Floats,  Up: Floating-point Functions

Combined Initialization and Assignment Functions
================================================

 - Macro: int mpfr_init_set (mpfr_t ROP, mpfr_t OP, mp_rnd_t RND)
 - Macro: int mpfr_init_set_ui (mpfr_t ROP, unsigned long int OP,
          mp_rnd_t RND)
 - Macro: int mpfr_init_set_si (mpfr_t ROP, signed long int OP,
          mp_rnd_t RND)
 - Macro: int mpfr_init_set_d (mpfr_t ROP, double OP, mp_rnd_t RND)
 - Macro: int mpfr_init_set_f (mpfr_t ROP, mpf_t OP, mp_rnd_t RND)
 - Macro: int mpfr_init_set_z (mpfr_t ROP, mpz_t OP, mp_rnd_t RND)
 - Macro: int mpfr_init_set_q (mpfr_t ROP, mpq_t OP, mp_rnd_t RND)
     Initialize ROP and set its value from OP, rounded to direction RND.
     The precision of ROP will be taken from the active default
     precision, as set by `mpfr_set_default_prec'.  The return value if
     zero if ROP=OP, positive if ROP>OP, and negative when ROP<OP.

 - Function: int mpfr_init_set_str (mpfr_t X, char *S, int BASE,
          mp_rnd_t RND)
     Initialize X and set its value from the string S in base BASE,
     rounded to direction RND.  See `mpfr_set_str'.


File: mpfr.info,  Node: Converting Floats,  Next: Float Arithmetic,  Prev: Simultaneous Float Init & Assign,  Up: Floating-point Functions

Conversion Functions
====================

 - Function: double mpfr_get_d (mpfr_t OP, mp_rnd_t RND)
     Convert OP to a double, using the rounding mode RND.

 - Function: double mpfr_get_d1 (mpfr_t OP)
     Convert OP to a double, using the default MPFR rounding mode (see
     function `mpfr_set_default_rounding_mode').

 - Function: mp_exp_t mpfr_get_z_exp (mpz_t Z, mpfr_t OP)
     Puts the mantissa of OP into Z, and returns the exponent EXP such
     that OP equals Z multiplied by two exponent EXP.

 - Function: char * mpfr_get_str (char *STR, mp_exp_t *EXPPTR, int
          BASE, size_t N_DIGITS, mpfr_t OP, mp_rnd_t RND)
     Convert OP to a string of digits in base BASE, with rounding in
     direction RND. The base may vary from 2 to 36.  Generate exactly
     N_DIGITS significant digits.

     If N_DIGITS is 0, it writes the maximum possible number of digits
     giving an exact rounding in the given base BASE with the direction
     RND. In other words, if OP was the exact rounding of a real number
     in direction RND, then the written value is also an exact rounding
     in base BASE of that real number with the same precision. An error
     occurs when one is unable to determine the leading digit, which
     can happen especially if the precision of OP is small.

     If STR is a null pointer, space for the mantissa is allocated using
     the default allocation function, and a pointer to the string is
     returned.  In that case, the user should her/himself free the
     corresponding memory with `(*_mp_free_func)(s, strlen(s) + 1)'.

     If STR is not a null pointer, it should point to a block of storage
     large enough for the mantissa, i.e., N_DIGITS + 2 or more. The
     extra two bytes are for a possible minus sign, and for the
     terminating null character.

     If the input number is a real number, the exponent is written
     through the pointer EXPPTR (the current minimal exponent for 0).

     If N_DIGITS is 0, note that the space requirements for STR in this
     case will be impossible for the user to predetermine. Therefore,
     one needs to pass a null pointer for the string argument whenever
     N_DIGITS is 0.

     The generated string is a fraction, with an implicit radix point
     immediately to the left of the first digit.  For example, the
     number 3.1416 would be returned as "31416" in the string and 1
     written at EXPPTR.

     A pointer to the string is returned, unless there is an error, in
     which case a null pointer is returned.


File: mpfr.info,  Node: Float Arithmetic,  Next: Float Comparison,  Prev: Converting Floats,  Up: Floating-point Functions

Basic Arithmetic Functions
==========================

 - Function: int mpfr_add (mpfr_t ROP, mpfr_t OP1, mpfr_t OP2, mp_rnd_t
          RND)
 - Function: int mpfr_add_ui (mpfr_t ROP, mpfr_t OP1, unsigned long int
          OP2, mp_rnd_t RND)
 - Function: int mpfr_add_z (mpfr_t ROP, mpfr_t OP1, mpz_t OP2,
          mp_rnd_t RND)
 - Function: int mpfr_add_q (mpfr_t ROP, mpfr_t OP1, mpq_t OP2,
          mp_rnd_t RND)
     Set ROP to OP1 + OP2 rounded in the direction RND.  The return
     value is zero if ROP is exactly OP1 + OP2, positive if ROP is
     larger than OP1 + OP2, and negative if ROP is smaller than OP1 +
     OP2.

 - Function: int mpfr_sub (mpfr_t ROP, mpfr_t OP1, mpfr_t OP2, mp_rnd_t
          RND)
 - Function: int mpfr_ui_sub (mpfr_t ROP, unsigned long int OP1, mpfr_t
          OP2, mp_rnd_t RND)
 - Function: int mpfr_sub_ui (mpfr_t ROP, mpfr_t OP1, unsigned long int
          OP2, mp_rnd_t RND)
 - Function: int mpfr_sub_z (mpfr_t ROP, mpfr_t OP1, mpz_t OP2,
          mp_rnd_t RND)
 - Function: int mpfr_sub_q (mpfr_t ROP, mpfr_t OP1, mpq_t OP2,
          mp_rnd_t RND)
     Set ROP to OP1 - OP2 rounded in the direction RND.  The return
     value is zero if ROP is exactly OP1 - OP2, positive if ROP is
     larger than OP1 - OP2, and negative if ROP is smaller than OP1 -
     OP2.

 - Function: int mpfr_mul (mpfr_t ROP, mpfr_t OP1, mpfr_t OP2, mp_rnd_t
          RND)
 - Function: int mpfr_mul_ui (mpfr_t ROP, mpfr_t OP1, unsigned long int
          OP2, mp_rnd_t RND)
 - Function: int mpfr_mul_z (mpfr_t ROP, mpfr_t OP1, mpz_t OP2,
          mp_rnd_t RND)
 - Function: int mpfr_mul_q (mpfr_t ROP, mpfr_t OP1, mpq_t OP2,
          mp_rnd_t RND)
     Set ROP to OP1 times OP2 rounded in the direction RND.  Return 0
     if the result is exact, a positive value if ROP>OP1*OP2, a
     negative value otherwise.

 - Function: int mpfr_div (mpfr_t ROP, mpfr_t OP1, mpfr_t OP2, mp_rnd_t
          RND)
 - Function: int mpfr_ui_div (mpfr_t ROP, unsigned long int OP1, mpfr_t
          OP2, mp_rnd_t RND)
 - Function: int mpfr_div_ui (mpfr_t ROP, mpfr_t OP1, unsigned long int
          OP2, mp_rnd_t RND)
 - Function: int mpfr_div_z (mpfr_t ROP, mpfr_t OP1, mpz_t OP2,
          mp_rnd_t RND)
 - Function: int mpfr_div_q (mpfr_t ROP, mpfr_t OP1, mpq_t OP2,
          mp_rnd_t RND)
     Set ROP to OP1/OP2 rounded in the direction RND.  These functions
     return 0 if the division is exact, a positive value when ROP is
     larger than OP1 divided by OP2, and a negative value otherwise.

 - Function: int mpfr_sqrt (mpfr_t ROP, mpfr_t OP, mp_rnd_t RND)
 - Function: int mpfr_sqrt_ui (mpfr_t ROP, unsigned long int OP,
          mp_rnd_t RND)
     Set ROP to the square root of OP rounded in the direction RND.
     Set ROP to NaN if OP is negative.  Return 0 if the operation is
     exact, a non-zero value otherwise.

 - Function: int mpfr_pow_ui (mpfr_t ROP, mpfr_t OP1, unsigned long int
          OP2, mp_rnd_t RND)
 - Function: int mpfr_ui_pow_ui (mpfr_t ROP, unsigned long int OP1,
          unsigned long int OP2, mp_rnd_t RND)
     Set ROP to OP1 raised to OP2. The computation is done by binary
     exponentiation.  Return 0 if the result is exact, a non-zero value
     otherwise (but the sign of the return value has no meaning).

 - Function: int mpfr_ui_pow (mpfr_t ROP, unsigned long int OP1, mpfr_t
          OP2, mp_rnd_t RND)
     Set ROP to OP1 raised to OP2, rounded to the direction RND with
     the precision of ROP.  Return zero iff the result is exact, a
     positive value when the result is greater than OP1 to the power
     OP2, and a negative value when it is smaller.

 - Function: int mpfr_pow_si (mpfr_t ROP, mpfr_t OP1, long int OP2,
          mp_rnd_t RND)
     Set ROP to OP1 raised to the power OP2, rounded to the direction
     RND with the precision of ROP.  Return zero iff the result is
     exact.

 - Function: int mpfr_pow (mpfr_t ROP, mpfr_t OP1, mpfr_t OP2, mp_rnd_t
          RND)
     Set ROP to OP1 raised to the power OP2, rounded to the direction
     RND with the precision of ROP.  If OP1 is negative then ROP is set
     to NaN, even if OP2 is an integer.  Return zero iff the result is
     exact.

 - Function: int mpfr_neg (mpfr_t ROP, mpfr_t OP, mp_rnd_t RND)
     Set ROP to -OP rounded in the direction RND.  Just changes the sign
     if ROP and OP are the same variable.

 - Function: int mpfr_abs (mpfr_t ROP, mpfr_t OP, mp_rnd_t RND)
     Set ROP to the absolute value of OP, rounded in the direction RND.
     Return 0 if the result is exact, a positive value if ROP is larger
     than the absolute value of OP, and a negative value otherwise.

 - Function: int mpfr_mul_2exp (mpfr_t ROP, mpfr_t OP1, unsigned long
          int OP2, mp_rnd_t RND)
 - Function: int mpfr_mul_2ui (mpfr_t ROP, mpfr_t OP1, unsigned long
          int OP2, mp_rnd_t RND)
 - Function: int mpfr_mul_2si (mpfr_t ROP, mpfr_t OP1, long int OP2,
          mp_rnd_t RND)
     Set ROP to OP1 times 2 raised to OP2 rounded to the direction RND.
     Just increases the exponent by OP2 when ROP and OP1 are identical.
     Return zero when ROP=OP1, a positive value when ROP>OP1, and a
     negative value when ROP<OP1.  Note: The `mpfr_mul_2exp' function
     is defined for compatibility reasons; you should use
     `mpfr_mul_2ui' (or `mpfr_mul_2si') instead.

 - Function: int mpfr_div_2exp (mpfr_t ROP, mpfr_t OP1, unsigned long
          int OP2, mp_rnd_t RND)
 - Function: int mpfr_div_2ui (mpfr_t ROP, mpfr_t OP1, unsigned long
          int OP2, mp_rnd_t RND)
 - Function: int mpfr_div_2si (mpfr_t ROP, mpfr_t OP1, long int OP2,
          mp_rnd_t RND)
     Set ROP to OP1 divided by 2 raised to OP2 rounded to the direction
     RND. Just decreases the exponent by OP2 when ROP and OP1 are
     identical.  Return zero when ROP=OP1, a positive value when
     ROP>OP1, and a negative value when ROP<OP1.  Note: The
     `mpfr_div_2exp' function is defined for compatibility reasons; you
     should use `mpfr_div_2ui' (or `mpfr_div_2si') instead.


File: mpfr.info,  Node: Float Comparison,  Next: I/O of Floats,  Prev: Float Arithmetic,  Up: Floating-point Functions

Comparison Functions
====================

 - Function: int mpfr_cmp (mpfr_t OP1, mpfr_t OP2)
 - Function: int mpfr_cmp_ui (mpfr_t OP1, unsigned long int OP2)
 - Function: int mpfr_cmp_si (mpfr_t OP1, signed long int OP2)
     Compare OP1 and OP2.  Return a positive value if OP1 > OP2, zero
     if OP1 = OP2, and a negative value if OP1 < OP2.  Both OP1 and OP2
     are considered to their full own precision, which may differ. In
     case OP1 and OP2 are of same sign but different, the absolute
     value returned is one plus the absolute difference of their
     exponents.  It is not allowed that one of the operands is NaN
     (Not-a-Number).

 - Function: int mpfr_cmp_ui_2exp (mpfr_t OP1, unsigned long int OP2,
          int E)
 - Function: int mpfr_cmp_si_2exp (mpfr_t OP1, long int OP2, int E)
     Compare OP1 and OP2 multiplied by two to the power E.

 - Function: int mpfr_eq (mpfr_t OP1, mpfr_t OP2, unsigned long int op3)
     Return non-zero if the first OP3 bits of OP1 and OP2 are equal,
     zero otherwise.  I.e., tests if OP1 and OP2 are approximately
     equal.

 - Function: int mpfr_nan_p (mpfr_t OP)
     Return non-zero if OP is Not-a-Number (NaN), zero otherwise.

 - Function: int mpfr_inf_p (mpfr_t OP)
     Return non-zero if OP is plus or minus infinity, zero otherwise.

 - Function: int mpfr_number_p (mpfr_t OP)
     Return non-zero if OP is an ordinary number, i.e. neither
     Not-a-Number nor plus or minus infinity.

 - Function: void mpfr_reldiff (mpfr_t ROP, mpfr_t OP1, mpfr_t OP2,
          mp_rnd_t RND)
     Compute the relative difference between OP1 and OP2 and store the
     result in ROP.  This function does not guarantee the exact
     rounding on the relative difference; it just computes
     abs(OP1-OP2)/OP1, using the rounding mode RND for all operations.

 - Function: int mpfr_sgn (mpfr_t OP)
     Return a positive value if OP > 0, zero if OP = 0, and a negative
     value if OP < 0.  Its result is not specified when OP is NaN
     (Not-a-Number).

Special Functions
=================

 - Function: int mpfr_log (mpfr_t ROP, mpfr_t OP, mp_rnd_t RND)
     Set ROP to the natural logarithm of OP, rounded to the direction
     RND with the precision of ROP.  Return zero when the result is
     exact (this occurs in fact only when OP is 0, 1, or +infinity) and
     a non-zero value otherwise (except for rounding to nearest, the
     sign of the return value is that of ROP-log(OP).

 - Function: int mpfr_exp (mpfr_t ROP, mpfr_t OP, mp_rnd_t RND)
     Set ROP to the exponential of OP, rounded to the direction RND
     with the precision of ROP.  Return zero when the result is exact
     (this occurs in fact only when OP is -infinity, 0, or +infinity),
     a positive value when the result is greater than the exponential
     of OP, and a negative value when it is smaller.

 - Function: int mpfr_exp2 (mpfr_t ROP, mpfr_t OP, mp_rnd_t RND)
     Set ROP to 2 power of OP, rounded to the direction RND with the
     precision of ROP.  Return zero iff the result is exact (this
     occurs in fact only when OP is -infinity, 0, or +infinity), a
     positive value when the result is greater than the exponential of
     OP, and a negative value when it is smaller.

 - Function: int mpfr_cos (mpfr_t COP, mpfr_t OP, mp_rnd_t RND)
 - Function: int mpfr_sin (mpfr_t SOP, mpfr_t OP, mp_rnd_t RND)
 - Function: int mpfr_tan (mpfr_t TOP, mpfr_t OP, mp_rnd_t RND)
     Set COP to the cosine of OP, SOP to the sine of OP, TOP to the
     tangent of OP, rounded to the direction RND with the precision of
     ROP. Return 0 iff the result is exact (this occurs in fact only
     when OP is 0 i.e. the sine is 0, the cosine is 1, and the tangent
     is 0).

 - Function: int mpfr_sin_cos (mpfr_t SOP, mpfr_t COP, mpfr_t OP,
          mp_rnd_t RND)
     Set simultaneously SOP to the sine of OP and
     COP to the cosine of OP, rounded to the direction RND with their
     corresponding precisions.  Return 0 iff both results are exact.

 - Function: int mpfr_acos (mpfr_t ROP, mpfr_t OP, mp_rnd_t RND)
 - Function: int mpfr_asin (mpfr_t ROP, mpfr_t OP, mp_rnd_t RND)
 - Function: int mpfr_atan (mpfr_t ROP, mpfr_t OP, mp_rnd_t RND)
     Set ROP to the arc-cosine, arc-sine or arc-tangent of OP, rounded
     to the direction RND with the precision of ROP.  Return 0 iff the
     result is exact.

 - Function: int mpfr_cosh (mpfr_t COP, mpfr_t OP, mp_rnd_t RND)
 - Function: int mpfr_sinh (mpfr_t SOP, mpfr_t OP, mp_rnd_t RND)
 - Function: int mpfr_tanh (mpfr_t TOP, mpfr_t OP, mp_rnd_t RND)
     Set COP to the hyperbolic cosine of OP,     SOP to the hyperbolic
     sine of OP,     TOP to the hyperbolic tangent of OP, rounded to
     the direction RND with the precision of ROP.  Return 0 iff the
     result is exact (this occurs in fact only when OP is 0 i.e. the
     result is 1).

 - Function: int mpfr_acosh (mpfr_t ROP, mpfr_t OP, mp_rnd_t RND)
 - Function: int mpfr_asinh (mpfr_t ROP, mpfr_t OP, mp_rnd_t RND)
 - Function: int mpfr_atanh (mpfr_t ROP, mpfr_t OP, mp_rnd_t RND)
     Set ROP to the inverse hyperbolic cosine, sine or tangent of OP,
     rounded to the direction RND with the precision of ROP.  Return 0
     iff the result is exact.

 - Function: int mpfr_fac_ui (mpfr_t ROP, unsigned long int OP,
          mp_rnd_t RND)
     Set ROP to the factorial of the unsigned long int OP, rounded to
     the direction RND with the precision of ROP.  Return 0 iff the
     result is exact.

 - Function: int mpfr_log1p (mpfr_t ROP, mpfr_t OP, mp_rnd_t RND)
     Set ROP to the logarithm of one plus OP, rounded to the direction
     RND with the precision of ROP.  Return 0 iff the result is exact
     (this occurs in fact only when OP is 0 i.e. the result is 0).

 - Function: int mpfr_expm1 (mpfr_t ROP, mpfr_t OP, mp_rnd_t RND)
     Set ROP to the exponential of OP minus one, rounded to the
     direction RND with the precision of ROP.  Return 0 iff the result
     is exact (this occurs in fact only when OP is 0 i.e. the result is
     0).

 - Function: int mpfr_log2 (mpfr_t ROP, mpfr_t OP, mp_rnd_t RND)
 - Function: int mpfr_log10 (mpfr_t ROP, mpfr_t OP, mp_rnd_t RND)
     Set ROP to the log[t] (t=2 or 10)(log x / log t) of OP, rounded to
     the direction RND with the precision of ROP. Return 0 iff the
     result is exact (this occurs in fact only when OP is 1 i.e. the
     result is 0).

 - Function: int mpfr_fma (mpfr_t ROP, mpfr_t OPX,mpfr_t OPY,mpfr_t
          OPZ, mp_rnd_t RND)
     Set ROP to OPX * OPY + OPZ, rounded to the direction RND with the
     precision of ROP. Return 0 iff the result is exact, a positive
     value if ROP is larger than OPX * OPY + OPZ, and a negative value
     otherwise.

 - Function: void mpfr_agm (mpfr_t ROP, mpfr_t OP1, mpfr_t OP2,
          mp_rnd_t RND)
     Set ROP to the arithmetic-geometric mean of OP1 and OP2, rounded
     to the direction RND with the precision of ROP.

 - Function: void mpfr_const_log2 (mpfr_t ROP, mp_rnd_t RND)
     Set ROP to the logarithm of 2 rounded to the direction RND with
     the precision of ROP. This function stores the computed value to
     avoid another calculation if a lower or equal precision is
     requested.

 - Function: void mpfr_const_pi (mpfr_t ROP, mp_rnd_t RND)
     Set ROP to the value of Pi rounded to the direction RND with the
     precision of ROP. This function uses the Borwein, Borwein, Plouffe
     formula which directly gives the expansion of Pi in base 16.

 - Function: void mpfr_const_euler (mpfr_t ROP, mp_rnd_t RND)
     Set ROP to the value of Euler's constant 0.577...  rounded to the
     direction RND with the precision of ROP.


File: mpfr.info,  Node: I/O of Floats,  Next: Miscellaneous Float Functions,  Prev: Float Comparison,  Up: Floating-point Functions

Input and Output Functions
==========================

   Functions that perform input from a standard input/output stream,
and functions that output to a standard input/output stream.  Passing a
null pointer for a STREAM argument to any of these functions will make
them read from `stdin' and write to `stdout', respectively.

   When using any of these functions, it is a good idea to include
`stdio.h' before `mpfr.h', since that will allow `mpfr.h' to define
prototypes for these functions.

 - Function: size_t mpfr_out_str (FILE *STREAM, int BASE, size_t
          N_DIGITS, mpfr_t OP, mp_rnd_t RND)
     Output OP on stdio stream STREAM, as a string of digits in base
     BASE, rounded to direction RND.  The base may vary from 2 to 36.
     Print at most N_DIGITS significant digits, or if N_DIGITS is 0,
     the maximum number of digits accurately representable by OP.

     In addition to the significant digits, a decimal point at the
     right of the first digit and a trailing exponent, in the form
     `eNNN', are printed.  If BASE is greater than 10, `@' will be used
     instead of `e' as exponent delimiter.

     Return the number of bytes written, or if an error occurred,
     return 0.

 - Function: size_t mpfr_inp_str (mpfr_t ROP, FILE *STREAM, int BASE,
          mp_rnd_t RND)
     Input a string in base BASE from stdio stream STREAM, rounded in
     direction RND, and put the read float in ROP.  The string is of
     the form `M@N' or, if the base is 10 or less, alternatively `MeN'
     or `MEN'.  `M' is the mantissa and `N' is the exponent.  The
     mantissa is always in the specified base.  The exponent is in
     decimal.

     The argument BASE may be in the range 2 to 36.

     Unlike the corresponding `mpz' function, the base will not be
     determined from the leading characters of the string if BASE is 0.
     This is so that numbers like `0.23' are not interpreted as octal.

     Return the number of bytes read, or if an error occurred, return 0.

 - Function: void mpfr_print_binary (mpfr_t FLOAT)
     Output FLOAT on stdout in raw binary format (the exponent is in
     decimal, yet).  The last bits from the least significant limb
     which do not belong to the mantissa are printed between square
     brackets; they should always be zero.


File: mpfr.info,  Node: Miscellaneous Float Functions,  Prev: I/O of Floats,  Up: Floating-point Functions

Miscellaneous Functions
=======================

 - Function: int mpfr_rint (mpfr_t ROP, mpfr_t OP, mp_rnd_t RND)
 - Function: int mpfr_ceil (mpfr_t ROP, mpfr_t OP)
 - Function: int mpfr_floor (mpfr_t ROP, mpfr_t OP)
 - Function: int mpfr_round (mpfr_t ROP, mpfr_t OP)
 - Function: int mpfr_trunc (mpfr_t ROP, mpfr_t OP)
     Set ROP to OP rounded to an integer. `mpfr_ceil' rounds to the
     next higher representable integer, `mpfr_floor' to the next lower,
     `mpfr_round' to the nearest representable integer, rounding
     halfway cases away from zero, and `mpfr_trunc' to the
     representable integer towards zero. `mpfr_rint' behaves like one
     of these four functions, depending on the rounding mode.  The
     returned value is zero when the result is exact, positive when it
     is greater than the original value of OP, and negative when it is
     smaller.  More precisely, the returned value is 0 when OP is an
     integer representable in ROP, 1 or -1 when OP is an integer that
     is not representable in ROP, 2 or -2 when OP is not an integer.

 - Function: void mpfr_urandomb (mpfr_t ROP, gmp_randstate_t STATE)
     Generate a uniformly distributed random float in the interval 0 <=
     X < 1.

 - Function: void mpfr_random (mpfr_t ROP)
     Generate a uniformly distributed random float in the interval 0 <=
     X < 1.

 - Function: void mpfr_random2 (mpfr_t ROP, mp_size_t MAX_SIZE,
          mp_exp_t MAX_EXP)
     Generate a random float of at most MAX_SIZE limbs, with long
     strings of zeros and ones in the binary representation. The
     exponent of the number is in the interval -EXP to EXP.  This
     function is useful for testing functions and algorithms, since
     this kind of random numbers have proven to be more likely to
     trigger corner-case bugs.  Negative random numbers are generated
     when MAX_SIZE is negative.

Internals
=========

   These types and functions were mainly designed for the
implementation of `mpfr', but may be useful for users too.  However no
upward compatibility is guaranteed.  You need to include `mpfr-impl.h'
to use them.

   The `mpfr_t' type consists of four fields.  The `_mpfr_prec' field
is used to store the precision of the variable (in bits); this is not
less than 2.

   The `_mpfr_size' field is used to store the number of allocated
limbs, with the high bits reserved to store the sign (bit 31), the NaN
flag (bit 30), and the Infinity flag (bit 29); thus bits 0 to 28 remain
for the number of allocated limbs, with a maximal value of 536870911.
A NaN is indicated by the NaN flag set, and no other fields are
relevant.  An Infinity is indicated by the NaN flag clear and the Inf
flag set; the sign bit of an Infinity indicates the sign, the limb data
and the exponent are not relevant.

   The `_mpfr_exp' field stores the exponent.  An exponent of 0 means a
radix point just above the most significant limb.  Non-zero values are
a multiplier 2^n relative to that point.

   Finally, the `_mpfr_d' is a pointer to the limbs, least significant
limbs stored first.  The number zero is represented with its most
significant limb set to zero, i.e. `_mpfr_d[n-1]' where
n=ceil(`_mpfr_prec'/`BITS_PER_MP_LIMB').  The number of limbs in use is
controlled by `_mpfr_prec', namely
ceil(`_mpfr_prec'/`BITS_PER_MP_LIMB').  Zero is represented by the most
significant limb being zero, other limb data and the exponent are not
relevant ("not relevant" implies that the corresponding objects may
contain invalid values, thus should not be evaluated even if they are
not taken into account).  Non-zero values always have the most
significant bit of the most significant limb set to 1.  When the
precision is not a whole number of limbs, the excess bits at the low
end of the data are zero.  When the precision has been lowered by
`mpfr_set_prec', the space allocated at `_mpfr_d' remains as given by
`_mpfr_size', but `_mpfr_prec' indicates how much of that space is
actually used.

 - Function: int mpfr_add_one_ulp (mpfr_t X, mp_rnd_t RND)
     Add one unit in last place (ulp) to X if X is finite and positive,
     subtract one ulp if X is finite and negative; otherwise, X is not
     changed.  The return value is zero unless an overflow occurs, in
     which case the `mpfr_add_one_ulp' function behaves like a
     conventional addition.

 - Function: int mpfr_sub_one_ulp (mpfr_t X, mp_rnd_t RND)
     Subtract one ulp to X if X is finite and positive, add one ulp if
     X is finite and negative; otherwise, X is not changed.  The return
     value is zero unless an underflow occurs, in which case the
     `mpfr_sub_one_ulp' function behaves like a conventional
     subtraction.

 - Function: int mpfr_can_round (mpfr_t B, mp_exp_t ERR, mp_rnd_t RND1,
          mp_rnd_t RND2, mp_prec_t PREC)
     Assuming B is an approximation of an unknown number X in direction
     RND1 with error at most two to the power E(b)-ERR where E(b) is
     the exponent of B, returns 1 if one is able to round exactly X to
     precision PREC with direction RND2,    and 0 otherwise. This
     function *does not modify* its arguments.


File: mpfr.info,  Node: Contributors,  Next: References,  Prev: Floating-point Functions,  Up: Top

Contributors
************

   The main developers consist of Guillaume Hanrot, Vincent Lefèvre and
Paul Zimmermann.

   We would like to thank Jean-Michel Muller and Joris van der Hoeven
for very fruitful discussions at the beginning of that project,
Torbjorn Granlund and Kevin Ryde for their help about design issues and
their suggestions for an easy integration into GNU MP, and Nathalie
Revol for her careful reading of this documentation.

   Sylvie Boldo from ENS-Lyon, France, contributed the functions
`mpfr_agm' and `mpfr_log'.  Emmanuel Jeandel, from ENS-Lyon too,
contributed the generic hypergeometric code in `generic.c', as well as
the `mpfr_exp3', a first implementation of the sine and cosine, and
improved versions of `mpfr_const_log2' and `mpfr_const_pi'.  Mathieu
Dutour contributed the functions `mpfr_atan' and `mpfr_asin', David
Daney contributed the hyperbolic and inverse hyperbolic functions, the
base-2 exponential, and the factorial function. Fabrice Rouillier
contributed the original version of `mul_ui.c', the `gmp_op.c' file,
and helped to the Windows porting.


File: mpfr.info,  Node: References,  Next: Concept Index,  Prev: Contributors,  Up: Top

References
**********

   * Torbjorn Granlund, "GNU MP: The GNU Multiple Precision Arithmetic
     Library",   version 4.0.1, 2001.

   * IEEE standard for binary floating-point arithmetic, Technical
     Report ANSI-IEEE Standard 754-1985, New York, 1985.  Approved
     March 21, 1985: IEEE Standards Board; approved July 26,   1985:
     American National Standards Institute, 18 pages.

   * Donald E. Knuth, "The Art of Computer Programming", vol 2,
     "Seminumerical Algorithms", 2nd edition, Addison-Wesley, 1981.



File: mpfr.info,  Node: Concept Index,  Next: Function Index,  Prev: References,  Up: Top

Concept Index
*************

* Menu:

* Arithmetic functions:                  Float Arithmetic.
* Comparison functions:                  Float Comparison.
* Conditions for copying MPFR:           Copying.
* Conversion functions:                  Converting Floats.
* Copying conditions:                    Copying.
* Float arithmetic functions:            Float Arithmetic.
* Float assignment functions:            Assigning Floats.
* Float comparisons functions:           Float Comparison.
* Float functions:                       Floating-point Functions.
* Float input and output functions:      I/O of Floats.
* Floating-point functions:              Floating-point Functions.
* Floating-point number:                 MPFR Basics.
* I/O functions:                         I/O of Floats.
* Initialization and assignment functions: Simultaneous Float Init & Assign.
* Input functions:                       I/O of Floats.
* Installation:                          Installing MPFR.
* Limb:                                  MPFR Basics.
* Miscellaneous float functions:         Miscellaneous Float Functions.
* mpfr.h:                                MPFR Basics.
* Output functions:                      I/O of Floats.
* Precision:                             MPFR Basics.
* Reporting bugs:                        Reporting Bugs.
* Rounding Mode:                         MPFR Basics.
* Rounding modes:                        Rounding Modes.
* Special functions:                     Float Comparison.
* User-defined precision:                Floating-point Functions.


File: mpfr.info,  Node: Function Index,  Prev: Concept Index,  Up: Top

Function and Type Index
***********************

* Menu:

* mp_prec_t:                             MPFR Basics.
* mp_rnd_t:                              MPFR Basics.
* mpfr_abs:                              Float Arithmetic.
* mpfr_acos:                             Float Comparison.
* mpfr_acosh:                            Float Comparison.
* mpfr_add:                              Float Arithmetic.
* mpfr_add_one_ulp:                      Miscellaneous Float Functions.
* mpfr_add_q:                            Float Arithmetic.
* mpfr_add_ui:                           Float Arithmetic.
* mpfr_add_z:                            Float Arithmetic.
* mpfr_agm:                              Float Comparison.
* mpfr_asin:                             Float Comparison.
* mpfr_asinh:                            Float Comparison.
* mpfr_atan:                             Float Comparison.
* mpfr_atanh:                            Float Comparison.
* mpfr_can_round:                        Miscellaneous Float Functions.
* mpfr_ceil:                             Miscellaneous Float Functions.
* mpfr_check_range:                      Exceptions.
* mpfr_clear:                            Initializing Floats.
* mpfr_clear_flags:                      Exceptions.
* mpfr_clear_inexflag:                   Exceptions.
* mpfr_clear_nanflag:                    Exceptions.
* mpfr_clear_overflow:                   Exceptions.
* mpfr_clear_underflow:                  Exceptions.
* mpfr_cmp:                              Float Comparison.
* mpfr_cmp_si:                           Float Comparison.
* mpfr_cmp_si_2exp:                      Float Comparison.
* mpfr_cmp_ui:                           Float Comparison.
* mpfr_cmp_ui_2exp:                      Float Comparison.
* mpfr_const_euler:                      Float Comparison.
* mpfr_const_log2:                       Float Comparison.
* mpfr_const_pi:                         Float Comparison.
* mpfr_cos:                              Float Comparison.
* mpfr_cosh:                             Float Comparison.
* mpfr_div:                              Float Arithmetic.
* mpfr_div_2exp:                         Float Arithmetic.
* mpfr_div_2si:                          Float Arithmetic.
* mpfr_div_2ui:                          Float Arithmetic.
* mpfr_div_q:                            Float Arithmetic.
* mpfr_div_ui:                           Float Arithmetic.
* mpfr_div_z:                            Float Arithmetic.
* mpfr_eq:                               Float Comparison.
* mpfr_exp:                              Float Comparison.
* mpfr_exp2:                             Float Comparison.
* mpfr_expm1:                            Float Comparison.
* mpfr_fac_ui:                           Float Comparison.
* mpfr_floor:                            Miscellaneous Float Functions.
* mpfr_fma:                              Float Comparison.
* mpfr_get_d:                            Converting Floats.
* mpfr_get_d1:                           Converting Floats.
* mpfr_get_default_prec:                 Initializing Floats.
* mpfr_get_emax:                         Exceptions.
* mpfr_get_emin:                         Exceptions.
* mpfr_get_prec:                         Initializing Floats.
* mpfr_get_str:                          Converting Floats.
* mpfr_get_z_exp:                        Converting Floats.
* mpfr_inexflag_p:                       Exceptions.
* mpfr_inf_p:                            Float Comparison.
* mpfr_init:                             Initializing Floats.
* mpfr_init2:                            Initializing Floats.
* mpfr_init_set:                         Simultaneous Float Init & Assign.
* mpfr_init_set_d:                       Simultaneous Float Init & Assign.
* mpfr_init_set_f:                       Simultaneous Float Init & Assign.
* mpfr_init_set_q:                       Simultaneous Float Init & Assign.
* mpfr_init_set_si:                      Simultaneous Float Init & Assign.
* mpfr_init_set_str:                     Simultaneous Float Init & Assign.
* mpfr_init_set_ui:                      Simultaneous Float Init & Assign.
* mpfr_init_set_z:                       Simultaneous Float Init & Assign.
* mpfr_inp_str:                          I/O of Floats.
* mpfr_log:                              Float Comparison.
* mpfr_log10:                            Float Comparison.
* mpfr_log1p:                            Float Comparison.
* mpfr_log2:                             Float Comparison.
* mpfr_mul:                              Float Arithmetic.
* mpfr_mul_2exp:                         Float Arithmetic.
* mpfr_mul_2si:                          Float Arithmetic.
* mpfr_mul_2ui:                          Float Arithmetic.
* mpfr_mul_q:                            Float Arithmetic.
* mpfr_mul_ui:                           Float Arithmetic.
* mpfr_mul_z:                            Float Arithmetic.
* mpfr_nan_p:                            Float Comparison.
* mpfr_nanflag_p:                        Exceptions.
* mpfr_neg:                              Float Arithmetic.
* mpfr_number_p:                         Float Comparison.
* mpfr_out_str:                          I/O of Floats.
* mpfr_overflow_p:                       Exceptions.
* mpfr_pow:                              Float Arithmetic.
* mpfr_pow_si:                           Float Arithmetic.
* mpfr_pow_ui:                           Float Arithmetic.
* mpfr_print_binary:                     I/O of Floats.
* mpfr_print_rnd_mode:                   Rounding Modes.
* mpfr_random:                           Miscellaneous Float Functions.
* mpfr_random2:                          Miscellaneous Float Functions.
* mpfr_reldiff:                          Float Comparison.
* mpfr_rint:                             Miscellaneous Float Functions.
* mpfr_round:                            Miscellaneous Float Functions.
* mpfr_round_prec:                       Rounding Modes.
* mpfr_set:                              Assigning Floats.
* mpfr_set_d:                            Assigning Floats.
* mpfr_set_default_prec:                 Initializing Floats.
* mpfr_set_default_rounding_mode:        Rounding Modes.
* mpfr_set_emax:                         Exceptions.
* mpfr_set_emin:                         Exceptions.
* mpfr_set_f:                            Assigning Floats.
* mpfr_set_inf:                          Assigning Floats.
* mpfr_set_machine_rnd_mode:             Rounding Modes.
* mpfr_set_nan:                          Assigning Floats.
* mpfr_set_prec:                         Initializing Floats.
* mpfr_set_prec_raw:                     Initializing Floats.
* mpfr_set_q:                            Assigning Floats.
* mpfr_set_si:                           Assigning Floats.
* mpfr_set_str:                          Assigning Floats.
* mpfr_set_str_raw:                      Assigning Floats.
* mpfr_set_ui:                           Assigning Floats.
* mpfr_set_z:                            Assigning Floats.
* mpfr_sgn:                              Float Comparison.
* mpfr_sin:                              Float Comparison.
* mpfr_sin_cos:                          Float Comparison.
* mpfr_sinh:                             Float Comparison.
* mpfr_sqrt:                             Float Arithmetic.
* mpfr_sqrt_ui:                          Float Arithmetic.
* mpfr_sub:                              Float Arithmetic.
* mpfr_sub_one_ulp:                      Miscellaneous Float Functions.
* mpfr_sub_q:                            Float Arithmetic.
* mpfr_sub_ui:                           Float Arithmetic.
* mpfr_sub_z:                            Float Arithmetic.
* mpfr_swap:                             Assigning Floats.
* mpfr_t:                                MPFR Basics.
* mpfr_tan:                              Float Comparison.
* mpfr_tanh:                             Float Comparison.
* mpfr_trunc:                            Miscellaneous Float Functions.
* mpfr_ui_div:                           Float Arithmetic.
* mpfr_ui_pow:                           Float Arithmetic.
* mpfr_ui_pow_ui:                        Float Arithmetic.
* mpfr_ui_sub:                           Float Arithmetic.
* mpfr_underflow_p:                      Exceptions.
* mpfr_urandomb:                         Miscellaneous Float Functions.



Tag Table:
Node: Top1010
Node: Copying1677
Node: Introduction to MPFR3397
Node: Installing MPFR5133
Node: Reporting Bugs7665
Node: MPFR Basics9195
Node: Floating-point Functions13276
Node: Rounding Modes15114
Node: Exceptions18227
Node: Initializing Floats20496
Node: Assigning Floats24168
Node: Simultaneous Float Init & Assign27386
Node: Converting Floats28627
Node: Float Arithmetic31301
Node: Float Comparison37456
Node: I/O of Floats45234
Node: Miscellaneous Float Functions47671
Node: Contributors52903
Node: References54098
Node: Concept Index54714
Node: Function Index56376

End Tag Table
