Index

  1. General Questions:

   1.1 What is Wireshark?

   1.2 What's up with the name change? Is Wireshark a fork?

   1.3 Where can I get help?

   1.4 What kind of shark is Wireshark?

   1.5 How is Wireshark pronounced, spelled and capitalized?

   1.6 How much does Wireshark cost?

   1.7 But I just paid someone on eBay for a copy of Wireshark!
   Did I get ripped off?

   1.8 Can I use Wireshark commercially?

   1.9 Can I use Wireshark as part of my commercial product?

   1.10 What protocols are currently supported?

   1.11 Are there any plans to support {your favorite protocol}?

   1.12 Can Wireshark read capture files from {your favorite
   network analyzer}?

   1.13 What devices can Wireshark use to capture packets?

   1.14 Does Wireshark work on Windows Vista or Windows Server
   2008?

  2. Installing Wireshark:

   2.1 I installed the Wireshark RPM (or other package); why did
   it install TShark but not Wireshark?

  3. Building Wireshark:

   3.1 I have libpcap installed; why did the configure script not
   find pcap.h or bpf.h?

   3.2 Why do I get the error dftest_DEPENDENCIES was already
   defined in condition TRUE, which implies condition
   HAVE_PLUGINS_TRUE when I try to build Wireshark from SVN or a
   SVN snapshot?

   3.3 Why does the linker fail with a number of "Output line too
   long." messages followed by linker errors when I try to build
   Wireshark?

   3.4 When I try to build Wireshark on Solaris, why does the link
   fail complaining that plugin_list is undefined?

   3.5 When I try to build Wireshark on Windows, why does the
   build fail because of conflicts between winsock.h and
   winsock2.h?

  4. Starting Wireshark:

   4.1 Why does Wireshark crash with a Bus Error when I try to run
   it on Solaris 8?

   4.2 When I try to run Wireshark, why does it complain about
   sprint_realloc_objid being undefined?

   4.3 I've installed Wireshark from Fink on OS X; why is it very
   slow to start up?

  5. Crashes and other fatal errors:

   5.1 I have an XXX network card on my machine; if I try to
   capture on it, why does my machine crash or reset itself?

   5.2 Why does my machine crash or reset itself when I select
   "Start" from the "Capture" menu or select "Preferences" from
   the "Edit" menu?

  6. Capturing packets:

   6.1 When I use Wireshark to capture packets, why do I see only
   packets to and from my machine, or not see all the traffic I'm
   expecting to see from or to the machine I'm trying to monitor?

   6.2 When I capture with Wireshark, why can't I see any TCP
   packets other than packets to and from my machine, even though
   another analyzer on the network sees those packets?

   6.3 Why am I only seeing ARP packets when I try to capture
   traffic?

   6.4 Why am I not seeing any traffic when I try to capture
   traffic?

   6.5 Can Wireshark capture on (my T1/E1 line, SS7 links, etc.)?

   6.6 How do I put an interface into promiscuous mode?

   6.7 I can set a display filter just fine; why don't capture
   filters work?

   6.8 I'm entering valid capture filters; why do I still get
   "parse error" errors?

   6.9 How can I capture packets with CRC errors?

   6.10 How can I capture entire frames, including the FCS?

   6.11 I'm capturing packets on a machine on a VLAN; why don't
   the packets I'm capturing have VLAN tags?

   6.12 Why does Wireshark hang after I stop a capture?

  7. Capturing packets on Windows:

   7.1 I'm running Wireshark on Windows; why does some network
   interface on my machine not show up in the list of interfaces
   in the "Interface:" field in the dialog box popped up by
   "Capture->Start", and/or why does Wireshark give me an error if
   I try to capture on that interface?

   7.2 I'm running Wireshark on Windows; why do no network
   interfaces show up in the list of interfaces in the
   "Interface:" field in the dialog box popped up by
   "Capture->Start"?

   7.3 I'm running Wireshark on Windows; why doesn't my serial
   port/ADSL modem/ISDN modem show up in the list of interfaces in
   the "Interface:" field in the dialog box popped up by
   "Capture->Start"?

   7.4 I'm running Wireshark on Windows NT 4.0/Windows
   2000/Windows XP/Windows Server 2003; my machine has a PPP
   (dial-up POTS, ISDN, etc.) interface, and it shows up in the
   "Interface" item in the "Capture Options" dialog box. Why can
   no packets be sent on or received from that network while I'm
   trying to capture traffic on that interface?

   7.5 I'm running Wireshark on Windows; why am I not seeing any
   traffic being sent by the machine running Wireshark?

   7.6 When I capture on Windows in promiscuous mode, I can see
   packets other than those sent to or from my machine; however,
   those packets show up with a "Short Frame" indication, unlike
   packets to or from my machine. What should I do to arrange that
   I see those packets in their entirety?

   7.7 I'm trying to capture 802.11 traffic on Windows; why am I
   not seeing any packets?

   7.8 I'm trying to capture 802.11 traffic on Windows; why am I
   seeing packets received by the machine on which I'm capturing
   traffic, but not packets sent by that machine?

   7.9 I'm trying to capture Ethernet VLAN traffic on Windows, and
   I'm capturing on a "raw" Ethernet device rather than a "VLAN
   interface", so that I can see the VLAN headers; why am I seeing
   packets received by the machine on which I'm capturing traffic,
   but not packets sent by that machine?

  8. Capturing packets on UN*Xes:

   8.1 I'm running Wireshark on a UNIX-flavored OS; why does some
   network interface on my machine not show up in the list of
   interfaces in the "Interface:" field in the dialog box popped
   up by "Capture->Start", and/or why does Wireshark give me an
   error if I try to capture on that interface?

   8.2 I'm running Wireshark on a UNIX-flavored OS; why do no
   network interfaces show up in the list of interfaces in the
   "Interface:" field in the dialog box popped up by
   "Capture->Start"?

   8.3 I'm capturing packets on Linux; why do the time stamps have
   only 100ms resolution, rather than 1us resolution?

  9. Capturing packets on wireless LANs:

   9.1 How can I capture raw 802.11 frames, including non-data
   (management, beacon) frames?

   9.2 How do I capture on an 802.11 device in monitor mode?

  10. Viewing traffic:

   10.1 Why am I seeing lots of packets with incorrect TCP
   checksums?

   10.2 I've just installed Wireshark, and the traffic on my local
   LAN is boring. Where can I find more interesting captures?

   10.3 Why doesn't Wireshark correctly identify RTP packets? It
   shows them only as UDP.

   10.4 Why doesn't Wireshark show Yahoo Messenger packets in
   captures that contain Yahoo Messenger traffic?

  11. Filtering traffic:

   11.1 I saved a filter and tried to use its name to filter the
   display; why do I get an "Unexpected end of filter string"
   error?

   11.2 How can I search for, or filter, packets that have a
   particular string anywhere in them?

   11.3 How do I filter a capture to see traffic for virus XXX?

  1. General Questions

   Q 1.1: What is Wireshark?

   A: Wireshark® is a network protocol analyzer. It lets you
   capture and interactively browse the traffic running on a
   computer network. It has a rich and powerful feature set and is
   world's most popular tool of its kind. It runs on most
   computing platforms including Windows, OS X, Linux, and UNIX.
   Network professionals, security experts, developers, and
   educators around the world use it regularly. It is freely
   available as open source, and is released under the GNU General
   Public License version 2.
   It is developed and maintained by a global team of protocol
   experts, and it is an example of a disruptive technology.
   Wireshark used to be known as Ethereal®. See the next question
   for details about the name change. If you're still using
   Ethereal, it is strongly recommended that you upgrade to
   Wireshark as Ethereal is unsupported and has known security
   vulnerabilities.
   For more information, please see the About Wireshark page.

   Q 1.2: What's up with the name change? Is Wireshark a fork?

   A: In May of 2006, Gerald Combs (the original author of
   Ethereal) went to work for CACE Technologies (best known for
   WinPcap). Unfortunately, he had to leave the Ethereal
   trademarks behind.
   This left the project in an awkward position. The only
   reasonable way to ensure the continued success of the project
   was to change the name. This is how Wireshark was born.
   Wireshark is almost (but not quite) a fork. Normally a "fork"
   of an open source project results in two names, web sites,
   development teams, support infrastructures, etc. This is the
   case with Wireshark except for one notable exception -- every
   member of the core development team is now working on
   Wireshark. There has been no active development on Ethereal
   since the name change. Several parts of the Ethereal web site
   (such as the mailing lists, source code repository, and build
   farm) have gone offline.
   More information on the name change can be found here:

     * Original press release
     * NewsForge article
     * Many other articles in our bibliography

   Q 1.3: Where can I get help?

   A: Community support is available on the Q&A site and on the
   wireshark-users mailing list. Subscription information and
   archives for all of Wireshark's mailing lists can be found at
   https://www.wireshark.org/mailman/listinfo. An IRC channel
   dedicated to Wireshark can be found at
   irc://irc.freenode.net/wireshark.
   Self-paced and instructor-led training is available at
   Wireshark University. Wireshark University also offers
   certification via the Wireshark Certified Network Analyst
   program.

   Q 1.4: What kind of shark is Wireshark?

   A: carcharodon photoshopia.

   Q 1.5: How is Wireshark pronounced, spelled and capitalized?

   A: Wireshark is pronounced as the word wire followed
   immediately by the word shark. Exact pronunciation and emphasis
   may vary depending on your locale (e.g. Arkansas).
   It's spelled with a capital W, followed by a lower-case
   ireshark. It is not a CamelCase word, i.e., WireShark is
   incorrect.

   Q 1.6: How much does Wireshark cost?

   A: Wireshark is "free software"; you can download it without
   paying any license fee. The version of Wireshark you download
   isn't a "demo" version, with limitations not present in a
   "full" version; it is the full version.
   The license under which Wireshark is issued is the GNU General
   Public License version 2. See the GNU GPL FAQ for some more
   information.

   Q 1.7: But I just paid someone on eBay for a copy of Wireshark!
   Did I get ripped off?

   A: That depends. Did they provide any sort of value-added
   product or service, such as installation support, installation
   media, training, trace file analysis, or funky-colored
   shark-themed socks? Probably not.
   Wireshark is available for anyone to download, absolutely free,
   at any time. Paying for a copy implies that you should get
   something for your money.

   Q 1.8: Can I use Wireshark commercially?

   A: Yes, if, for example, you mean "I work for a commercial
   organization; can I use Wireshark to capture and analyze
   network traffic in our company's networks or in our customer's
   networks?"
   If you mean "Can I use Wireshark as part of my commercial
   product?", see the next entry in the FAQ.

   Q 1.9: Can I use Wireshark as part of my commercial product?

   A: As noted, Wireshark is licensed under the GNU General Public
   License, version 2. The GPL imposes conditions on your use of
   GPL'ed code in your own products; you cannot, for example, make
   a "derived work" from Wireshark, by making modifications to it,
   and then sell the resulting derived work and not allow
   recipients to give away the resulting work. You must also make
   the changes you've made to the Wireshark source available to
   all recipients of your modified version; those changes must
   also be licensed under the terms of the GPL. See the GPL FAQ
   for more details; in particular, note the answer to the
   question about modifying a GPLed program and selling it
   commercially, and the question about linking GPLed code with
   other code to make a proprietary program.
   You can combine a GPLed program such as Wireshark and a
   commercial program as long as they communicate "at arm's
   length", as per this item in the GPL FAQ.
   We recommend keeping Wireshark and your product completely
   separate, communicating over sockets or pipes. If you're
   loading any part of Wireshark as a DLL, you're probably doing
   it wrong.

   Q 1.10: What protocols are currently supported?

   A: There are currently hundreds of supported protocols and
   media. Details can be found in the wireshark(1) man page.

   Q 1.11: Are there any plans to support {your favorite
   protocol}?

   A: Support for particular protocols is added to Wireshark as a
   result of people contributing that support; no formal plans for
   adding support for particular protocols in particular future
   releases exist.

   Q 1.12: Can Wireshark read capture files from {your favorite
   network analyzer}?

   A: Support for particular capture file formats is added to
   Wireshark as a result of people contributing that support; no
   formal plans for adding support for particular capture file
   formats in particular future releases exist.
   If a network analyzer writes out files in a format already
   supported by Wireshark (e.g., in libpcap format), Wireshark may
   already be able to read them, unless the analyzer has added its
   own proprietary extensions to that format.
   If a network analyzer writes out files in its own format, or
   has added proprietary extensions to another format, in order to
   make Wireshark read captures from that network analyzer, we
   would either have to have a specification for the file format,
   or the extensions, sufficient to give us enough information to
   read the parts of the file relevant to Wireshark, or would need
   at least one capture file in that format AND a detailed textual
   analysis of the packets in that capture file (showing packet
   time stamps, packet lengths, and the top-level packet header)
   in order to reverse-engineer the file format.
   Note that there is no guarantee that we will be able to
   reverse-engineer a capture file format.

   Q 1.13: What devices can Wireshark use to capture packets?

   A: Wireshark can read live data from Ethernet, Token-Ring,
   FDDI, serial (PPP and SLIP) (if the OS on which it's running
   allows Wireshark to do so), 802.11 wireless LAN (if the OS on
   which it's running allows Wireshark to do so), ATM connections
   (if the OS on which it's running allows Wireshark to do so),
   and the "any" device supported on Linux by recent versions of
   libpcap.
   See the list of supported capture media on various OSes for
   details (several items in there say "Unknown", which doesn't
   mean "Wireshark can't capture on them", it means "we don't know
   whether it can capture on them"; we expect that it will be able
   to capture on many of them, but we haven't tried it ourselves -
   if you try one of those types and it works, please update the
   wiki page accordingly.
   It can also read a variety of capture file formats, including:

     * AG Group/WildPackets/Savvius
       EtherPeek/TokenPeek/AiroPeek/EtherHelp/Packet Grabber
       captures
     * AIX's iptrace captures
     * Accellent's 5Views LAN agent output
     * Cinco Networks NetXRay captures
     * Cisco Secure Intrusion Detection System IPLog output
     * CoSine L2 debug output
     * DBS Etherwatch VMS text output
     * Endace Measurement Systems' ERF format captures
     * EyeSDN USB S0 traces
     * HP-UX nettl captures
     * ISDN4BSD project i4btrace captures
     * Linux Bluez Bluetooth stack hcidump -w traces
     * Lucent/Ascend router debug output
     * Microsoft Network Monitor captures
     * Network Associates Windows-based Sniffer captures
     * Network General/Network Associates DOS-based Sniffer
       (compressed or uncompressed) captures
     * Network Instruments Observer version 9 captures
     * Novell LANalyzer captures
     * RADCOM's WAN/LAN analyzer captures
     * Shomiti/Finisar Surveyor captures
     * Toshiba's ISDN routers dump output
     * VMS TCPIPtrace/TCPtrace/UCX$TRACE output
     * Visual Networks' Visual UpTime traffic capture
     * libpcap, tcpdump and various other tools using tcpdump's
       capture format
     * snoop and atmsnoop output

   so that it can read traces from various network types, as
   captured by other applications or equipment, even if it cannot
   itself capture on those network types.

   Q 1.14: Does Wireshark work on Windows Vista or Windows Server
   2008?

   A: Yes, but if you want to capture packets as a normal user,
   you must make sure npf.sys is loaded. Wireshark's installer
   enables this by default. This is not a concern if you run
   Wireshark as Administrator, but this is discouraged. See the
   CapturePrivileges page on the wiki for more details.

  2. Installing Wireshark

   Q 2.1: I installed the Wireshark RPM (or other package); why
   did it install TShark but not Wireshark?

   A: Many distributions have separate Wireshark packages, one for
   non-GUI components such as TShark, editcap, dumpcap, etc. and
   one for the GUI. If this is the case on your system, there's
   probably a separate package named wireshark-gnome or
   wireshark-gtk+. Find it and install it.

  3. Building Wireshark

   Q 3.1: I have libpcap installed; why did the configure script
   not find pcap.h or bpf.h?

   A: Are you sure pcap.h and bpf.h are installed? The official
   distribution of libpcap only installs the libpcap.a library
   file when "make install" is run. To install pcap.h and bpf.h,
   you must run "make install-incl". If you're running Debian or
   Redhat, make sure you have the "libpcap-dev" or "libpcap-devel"
   packages installed.
   It's also possible that pcap.h and bpf.h have been installed in
   a strange location. If this is the case, you may have to tweak
   aclocal.m4.

   Q 3.2: Why do I get the error dftest_DEPENDENCIES was already
   defined in condition TRUE, which implies condition
   HAVE_PLUGINS_TRUE when I try to build Wireshark from SVN or a
   SVN snapshot?

   A: You probably have automake 1.5 installed on your machine
   (the command automake --version will report the version of
   automake on your machine). There is a bug in that version of
   automake that causes this problem; upgrade to a later version
   of automake (1.6 or later).

   Q 3.3: Why does the linker fail with a number of "Output line
   too long." messages followed by linker errors when I try to
   build Wireshark?

   A: The version of the sed command on your system is incapable
   of handling very long lines. On Solaris, for example,
   /usr/bin/sed has a line length limit too low to allow libtool
   to work; /usr/xpg4/bin/sed can handle it, as can GNU sed if you
   have it installed.
   On Solaris, changing your command search path to search
   /usr/xpg4/bin before /usr/bin should make the problem go away;
   on any platform on which you have this problem, installing GNU
   sed and changing your command path to search the directory in
   which it is installed before searching the directory with the
   version of sed that came with the OS should make the problem go
   away.

   Q 3.4: When I try to build Wireshark on Solaris, why does the
   link fail complaining that plugin_list is undefined?

   A: This appears to be due to a problem with some versions of
   the GTK+ and GLib packages from www.sunfreeware.org; un-install
   those packages, and try getting the 1.2.10 versions from that
   site, or the versions from The Written Word, or the versions
   from Sun's GNOME distribution, or the versions from the
   supplemental software CD that comes with the Solaris media kit,
   or build them from source from the GTK Web site. Then re-run
   the configuration script, and try rebuilding Wireshark. (If you
   get the 1.2.10 versions from www.sunfreeware.org, and the
   problem persists, un-install them and try installing one of the
   other versions mentioned.)

   Q 3.5: When I try to build Wireshark on Windows, why does the
   build fail because of conflicts between winsock.h and
   winsock2.h?

   A: As of Wireshark 0.9.5, you must install WinPcap 2.3 or
   later, and the corresponding version of the developer's pack,
   in order to be able to compile Wireshark; it will not compile
   with older versions of the developer's pack. The symptoms of
   this failure are conflicts between definitions in winsock.h and
   in winsock2.h; Wireshark uses winsock2.h, but pre-2.3 versions
   of the WinPcap developer's packet use winsock.h. (2.3 uses
   winsock2.h, so if Wireshark were to use winsock.h, it would not
   be able to build with current versions of the WinPcap
   developer's pack.)
   Note that the installed version of the developer's pack should
   be the same version as the version of WinPcap you have
   installed.

  4. Starting Wireshark

   Q 4.1: Why does Wireshark crash with a Bus Error when I try to
   run it on Solaris 8?

   A: Some versions of the GTK+ library from www.sunfreeware.org
   appear to be buggy, causing Wireshark to drop core with a Bus
   Error. Un-install those packages, and try getting the 1.2.10
   version from that site, or the version from The Written Word,
   or the version from Sun's GNOME distribution, or the version
   from the supplemental software CD that comes with the Solaris
   media kit, or build it from source from the GTK Web site.
   Update the GLib library to the 1.2.10 version, from the same
   source, as well. (If you get the 1.2.10 versions from
   www.sunfreeware.org, and the problem persists, un-install them
   and try installing one of the other versions mentioned.)
   Similar problems may exist with older versions of GTK+ for
   earlier versions of Solaris.

   Q 4.2: When I try to run Wireshark, why does it complain about
   sprint_realloc_objid being undefined?

   A: Wireshark can only be linked with version 4.2.2 or later of
   UCD SNMP. Your version of Wireshark was dynamically linked with
   such a version of UCD SNMP; however, you have an older version
   of UCD SNMP installed, which means that when Wireshark is run,
   it tries to link to the older version, and fails. You will have
   to replace that version of UCD SNMP with version 4.2.2 or a
   later version.

   Q 4.3: I've installed Wireshark from Fink on OS X; why is it
   very slow to start up?

   A: When an application is installed on OS X, prior to 10.4, it
   is usually "prebound" to speed up launching the application.
   (That's what the "Optimizing" phase of installation is.)
   Fink normally performs prebinding automatically when you
   install a package. However, in some rare cases, for whatever
   reason the prebinding caches get corrupt, and then not only
   does prebinding fail, but startup actually becomes much slower,
   because the system tries in vain to perform prebinding "on the
   fly" as you launch the application. This fails, causing
   sometimes huge delays.
   To fix the prebinding caches, run the command



	sudo /sw/var/lib/fink/prebound/update-package-prebinding.pl -f



  5. Crashes and other fatal errors

   Q 5.1: I have an XXX network card on my machine; if I try to
   capture on it, why does my machine crash or reset itself?

   A: This is almost certainly a problem with one or more of:

     * the operating system you're using;
     * the device driver for the interface you're using;
     * the libpcap/WinPcap library and, if this is Windows, the
       WinPcap device driver;

   so:

     * if you are using Windows, see the WinPcap support page -
       check the "Submitting bugs" section;
     * if you are using some Linux distribution, some version of
       BSD, or some other UNIX-flavored OS, you should report the
       problem to the company or organization that produces the OS
       (in the case of a Linux distribution, report the problem to
       whoever produces the distribution).

   Q 5.2: Why does my machine crash or reset itself when I select
   "Start" from the "Capture" menu or select "Preferences" from
   the "Edit" menu?

   A: Both of those operations cause Wireshark to try to build a
   list of the interfaces that it can open; it does so by getting
   a list of interfaces and trying to open them. There is probably
   an OS, driver, or, for Windows, WinPcap bug that causes the
   system to crash when this happens; see the previous question.

  6. Capturing packets

   Q 6.1: When I use Wireshark to capture packets, why do I see
   only packets to and from my machine, or not see all the traffic
   I'm expecting to see from or to the machine I'm trying to
   monitor?

   A: This might be because the interface on which you're
   capturing is plugged into an Ethernet or Token Ring switch; on
   a switched network, unicast traffic between two ports will not
   necessarily appear on other ports - only broadcast and
   multicast traffic will be sent to all ports.
   Note that even if your machine is plugged into a hub, the "hub"
   may be a switched hub, in which case you're still on a switched
   network.
   Note also that on the Linksys Web site, they say that their
   auto-sensing hubs "broadcast the 10Mb packets to the port that
   operate at 10Mb only and broadcast the 100Mb packets to the
   ports that operate at 100Mb only", which would indicate that if
   you sniff on a 10Mb port, you will not see traffic coming sent
   to a 100Mb port, and vice versa. This problem has also been
   reported for Netgear dual-speed hubs, and may exist for other
   "auto-sensing" or "dual-speed" hubs.
   Some switches have the ability to replicate all traffic on all
   ports to a single port so that you can plug your analyzer into
   that single port to sniff all traffic. You would have to check
   the documentation for the switch to see if this is possible
   and, if so, to see how to do this. See the switch reference
   page on the Wireshark Wiki for information on some switches.
   (Note that it's a Wiki, so you can update or fix that
   information, or add additional information on those switches or
   information on new switches, yourself.)
   Note also that many firewall/NAT boxes have a switch built into
   them; this includes many of the "cable/DSL router" boxes. If
   you have a box of that sort, that has a switch with some number
   of Ethernet ports into which you plug machines on your network,
   and another Ethernet port used to connect to a cable or DSL
   modem, you can, at least, sniff traffic between the machines on
   your network and the Internet by plugging the Ethernet port on
   the router going to the modem, the Ethernet port on the modem,
   and the machine on which you're running Wireshark into a hub
   (make sure it's not a switching hub, and that, if it's a
   dual-speed hub, all three of those ports are running at the
   same speed.
   If your machine is not plugged into a switched network or a
   dual-speed hub, or it is plugged into a switched network but
   the port is set up to have all traffic replicated to it, the
   problem might be that the network interface on which you're
   capturing doesn't support "promiscuous" mode, or because your
   OS can't put the interface into promiscuous mode. Normally,
   network interfaces supply to the host only:

     * packets sent to one of that host's link-layer addresses;
     * broadcast packets;
     * multicast packets sent to a multicast address that the host
       has configured the interface to accept.

   Most network interfaces can also be put in "promiscuous" mode,
   in which they supply to the host all network packets they see.
   Wireshark will try to put the interface on which it's capturing
   into promiscuous mode unless the "Capture packets in
   promiscuous mode" option is turned off in the "Capture Options"
   dialog box, and TShark will try to put the interface on which
   it's capturing into promiscuous mode unless the -p option was
   specified. However, some network interfaces don't support
   promiscuous mode, and some OSes might not allow interfaces to
   be put into promiscuous mode.
   If the interface is not running in promiscuous mode, it won't
   see any traffic that isn't intended to be seen by your machine.
   It will see broadcast packets, and multicast packets sent to a
   multicast MAC address the interface is set up to receive.
   You should ask the vendor of your network interface whether it
   supports promiscuous mode. If it does, you should ask whoever
   supplied the driver for the interface (the vendor, or the
   supplier of the OS you're running on your machine) whether it
   supports promiscuous mode with that network interface.
   In the case of token ring interfaces, the drivers for some of
   them, on Windows, may require you to enable promiscuous mode in
   order to capture in promiscuous mode. See the Wireshark Wiki
   item on Token Ring capturing for details.
   In the case of wireless LAN interfaces, it appears that, when
   those interfaces are promiscuously sniffing, they're running in
   a significantly different mode from the mode that they run in
   when they're just acting as network interfaces (to the extent
   that it would be a significant effort for those drivers to
   support for promiscuously sniffing and acting as regular
   network interfaces at the same time), so it may be that Windows
   drivers for those interfaces don't support promiscuous mode.

   Q 6.2: When I capture with Wireshark, why can't I see any TCP
   packets other than packets to and from my machine, even though
   another analyzer on the network sees those packets?

   A: You're probably not seeing any packets other than unicast
   packets to or from your machine, and broadcast and multicast
   packets; a switch will normally send to a port only unicast
   traffic sent to the MAC address for the interface on that port,
   and broadcast and multicast traffic - it won't send to that
   port unicast traffic sent to a MAC address for some other
   interface - and a network interface not in promiscuous mode
   will receive only unicast traffic sent to the MAC address for
   that interface, broadcast traffic, and multicast traffic sent
   to a multicast MAC address the interface is set up to receive.
   TCP doesn't use broadcast or multicast, so you will only see
   your own TCP traffic, but UDP services may use broadcast or
   multicast so you'll see some UDP traffic - however, this is not
   a problem with TCP traffic, it's a problem with unicast
   traffic, as you also won't see all UDP traffic between other
   machines.
   I.e., this is probably the same question as this earlier one;
   see the response to that question.

   Q 6.3: Why am I only seeing ARP packets when I try to capture
   traffic?

   A: You're probably on a switched network, and running Wireshark
   on a machine that's not sending traffic to the switch and not
   being sent any traffic from other machines on the switch. ARP
   packets are often broadcast packets, which are sent to all
   switch ports.
   I.e., this is probably the same question as this earlier one;
   see the response to that question.

   Q 6.4: Why am I not seeing any traffic when I try to capture
   traffic?

   A: Is the machine running Wireshark sending out any traffic on
   the network interface on which you're capturing, or receiving
   any traffic on that network, or is there any broadcast traffic
   on the network or multicast traffic to a multicast group to
   which the machine running Wireshark belongs?
   If not, this may just be a problem with promiscuous sniffing,
   either due to running on a switched network or a dual-speed
   hub, or due to problems with the interface not supporting
   promiscuous mode; see the response to this earlier question.
   Otherwise, on Windows, see the response to this question and,
   on a UNIX-flavored OS, see the response to this question.

   Q 6.5: Can Wireshark capture on (my T1/E1 line, SS7 links,
   etc.)?

   A: Wireshark can only capture on devices supported by
   libpcap/WinPcap. On most OSes, only devices that can act as
   network interfaces of the type that support IP are supported as
   capture devices for libpcap/WinPcap, although the device
   doesn't necessarily have to be running as an IP interface in
   order to support traffic capture.
   On Linux and FreeBSD, libpcap 0.8 and later support the API for
   Endace Measurement Systems' DAG cards, so that a system with
   one of those cards, and its driver and libraries, installed can
   capture traffic with those cards with libpcap-based
   applications. You would either have to have a version of
   Wireshark built with that version of libpcap, or a
   dynamically-linked version of Wireshark and a shared libpcap
   library with DAG support, in order to do so with Wireshark. You
   should ask Endace whether that could be used to capture traffic
   on, for example, your T1/E1 link.
   See the SS7 capture setup page on the Wireshark Wiki for
   current information on capturing SS7 traffic on TDM links.

   Q 6.6: How do I put an interface into promiscuous mode?

   A: By not disabling promiscuous mode when running Wireshark or
   TShark.
   Note, however, that:

     * the form of promiscuous mode that libpcap (the library that
       programs such as tcpdump, Wireshark, etc. use to do packet
       capture) turns on will not necessarily be shown if you run
       ifconfig on the interface on a UNIX system;
     * some network interfaces might not support promiscuous mode,
       and some drivers might not allow promiscuous mode to be
       turned on - see this earlier question for more information
       on that;
     * the fact that you're not seeing any traffic, or are only
       seeing broadcast traffic, or aren't seeing any
       non-broadcast traffic other than traffic to or from the
       machine running Wireshark, does not mean that promiscuous
       mode isn't on - see this earlier question for more
       information on that.

   I.e., this is probably the same question as this earlier one;
   see the response to that question.

   Q 6.7: I can set a display filter just fine; why don't capture
   filters work?

   A: Capture filters currently use a different syntax than
   display filters. Here's the corresponding section from the
   wireshark(1) man page:
   "Display filters in Wireshark are very powerful; more fields
   are filterable in Wireshark than in other protocol analyzers,
   and the syntax you can use to create your filters is richer. As
   Wireshark progresses, expect more and more protocol fields to
   be allowed in display filters.
   Packet capturing is performed with the pcap library. The
   capture filter syntax follows the rules of the pcap library.
   This syntax is different from the display filter syntax."
   The capture filter syntax used by libpcap can be found in the
   tcpdump(8) man page.

   Q 6.8: I'm entering valid capture filters; why do I still get
   "parse error" errors?

   A: There is a bug in some versions of libpcap/WinPcap that
   cause it to report parse errors even for valid expressions if a
   previous filter expression was invalid and got a parse error.
   Try exiting and restarting Wireshark; if you are using a
   version of libpcap/WinPcap with this bug, this will "erase" its
   memory of the previous parse error. If the capture filter that
   got the "parse error" now works, the earlier error with that
   filter was probably due to this bug.
   The bug was fixed in libpcap 0.6; 0.4[.x] and 0.5[.x] versions
   of libpcap have this bug, but 0.6[.x] and later versions don't.
   Versions of WinPcap prior to 2.3 are based on pre-0.6 versions
   of libpcap, and have this bug; WinPcap 2.3 is based on libpcap
   0.6.2, and doesn't have this bug.
   If you are running Wireshark on a UNIX-flavored platform, run
   "wireshark -v", or select "About Wireshark..." from the "Help"
   menu in Wireshark, to see what version of libpcap it's using.
   If it's not 0.6 or later, you will need either to upgrade your
   OS to get a later version of libpcap, or will need to build and
   install a later version of libpcap from the tcpdump.org Web
   site and then recompile Wireshark from source with that later
   version of libpcap.
   If you are running Wireshark on Windows with a pre-2.3 version
   of WinPcap, you will need to un-install WinPcap and then
   download and install WinPcap 2.3.

   Q 6.9: How can I capture packets with CRC errors?

   A: Wireshark can capture only the packets that the packet
   capture library - libpcap on UNIX-flavored OSes, and the
   WinPcap port to Windows of libpcap on Windows - can capture,
   and libpcap/WinPcap can capture only the packets that the OS's
   raw packet capture mechanism (or the WinPcap driver, and the
   underlying OS networking code and network interface drivers, on
   Windows) will allow it to capture.
   Unless the OS always supplies packets with errors such as
   invalid CRCs to the raw packet capture mechanism, or can be
   configured to do so, invalid CRCs to the raw packet capture
   mechanism, Wireshark - and other programs that capture raw
   packets, such as tcpdump - cannot capture those packets. You
   will have to determine whether your OS needs to be so
   configured and, if so, can be so configured, configure it if
   necessary and possible, and make whatever changes to libpcap
   and the packet capture program you're using are necessary, if
   any, to support capturing those packets.
   Most OSes probably do not support capturing packets with
   invalid CRCs on Ethernet, and probably do not support it on
   most other link-layer types. Some drivers on some OSes do
   support it, such as some Ethernet drivers on FreeBSD; in those
   OSes, you might always get those packets, or you might only get
   them if you capture in promiscuous mode (you'd have to
   determine which is the case).
   Note that libpcap does not currently supply to programs that
   use it an indication of whether the packet's CRC was invalid
   (because the drivers themselves do not supply that information
   to the raw packet capture mechanism); therefore, Wireshark will
   not indicate which packets had CRC errors unless the FCS was
   captured (see the next question) and you're using Wireshark
   0.9.15 and later, in which case Wireshark will check the CRC
   and indicate whether it's correct or not.

   Q 6.10: How can I capture entire frames, including the FCS?

   A: Wireshark can only capture data that the packet capture
   library - libpcap on UNIX-flavored OSes, and the WinPcap port
   to Windows of libpcap on Windows - can capture, and
   libpcap/WinPcap can capture only the data that the OS's raw
   packet capture mechanism (or the WinPcap driver, and the
   underlying OS networking code and network interface drivers, on
   Windows) will allow it to capture.
   For any particular link-layer network type, unless the OS
   supplies the FCS of a frame as part of the frame, or can be
   configured to do so, Wireshark - and other programs that
   capture raw packets, such as tcpdump - cannot capture the FCS
   of a frame. You will have to determine whether your OS needs to
   be so configured and, if so, can be so configured, configure it
   if necessary and possible, and make whatever changes to libpcap
   and the packet capture program you're using are necessary, if
   any, to support capturing the FCS of a frame.
   Most OSes do not support capturing the FCS of a frame on
   Ethernet, and probably do not support it on most other
   link-layer types. Some drivres on some OSes do support it, such
   as some (all?) Ethernet drivers on NetBSD and possibly the
   driver for Apple's gigabit Ethernet interface in OS X; in those
   OSes, you might always get the FCS, or you might only get the
   FCS if you capture in promiscuous mode (you'd have to determine
   which is the case).
   Versions of Wireshark prior to 0.9.15 will not treat an
   Ethernet FCS in a captured packet as an FCS. 0.9.15 and later
   will attempt to determine whether there's an FCS at the end of
   the frame and, if it thinks there is, will display it as such,
   and will check whether it's the correct CRC-32 value or not.

   Q 6.11: I'm capturing packets on a machine on a VLAN; why don't
   the packets I'm capturing have VLAN tags?

   A: You might be capturing on what might be called a "VLAN
   interface" - the way a particular OS makes VLANs plug into the
   networking stack might, for example, be to have a network
   device object for the physical interface, which takes VLAN
   packets, strips off the VLAN header and constructs an Ethernet
   header, and passes that packet to an internal network device
   object for the VLAN, which then passes the packets onto various
   higher-level protocol implementations.
   In order to see the raw Ethernet packets, rather than
   "de-VLANized" packets, you would have to capture not on the
   virtual interface for the VLAN, but on the interface
   corresponding to the physical network device, if possible. See
   the Wireshark Wiki item on VLAN capturing for details.

   Q 6.12: Why does Wireshark hang after I stop a capture?

   A: The most likely reason for this is that Wireshark is trying
   to look up an IP address in the capture to convert it to a name
   (so that, for example, it can display the name in the source
   address or destination address columns), and that lookup
   process is taking a very long time.
   Wireshark calls a routine in the OS of the machine on which
   it's running to convert of IP addresses to the corresponding
   names. That routine probably does one or more of:

     * a search of a system file listing IP addresses and names;
     * a lookup using DNS;
     * on UNIX systems, a lookup using NIS;
     * on Windows systems, a NetBIOS-over-TCP query.

   If a DNS server that's used in an address lookup is not
   responding, the lookup will fail, but will only fail after a
   timeout while the system routine waits for a reply.
   In addition, on Windows systems, if the DNS lookup of the
   address fails, either because the server isn't responding or
   because there are no records in the DNS that could be used to
   map the address to a name, a NetBIOS-over-TCP query will be
   made. That query involves sending a message to the
   NetBIOS-over-TCP name service on that machine, asking for the
   name and other information about the machine. If the machine
   isn't running software that responds to those queries - for
   example, many non-Windows machines wouldn't be running that
   software - the lookup will only fail after a timeout. Those
   timeouts can cause the lookup to take a long time.
   If you disable network address-to-name translation - for
   example, by turning off the "Enable network name resolution"
   option in the "Capture Options" dialog box for starting a
   network capture - the lookups of the address won't be done,
   which may speed up the process of reading the capture file
   after the capture is stopped. You can make that setting the
   default by selecting "Preferences" from the "Edit" menu,
   turning off the "Enable network name resolution" option in the
   "Name resolution" options in the preferences disalog box, and
   using the "Save" button in that dialog box; note that this will
   save all your current preference settings.
   If Wireshark hangs when reading a capture even with network
   name resolution turned off, there might, for example, be a bug
   in one of Wireshark's dissectors for a protocol causing it to
   loop infinitely. If you're not running the most recent release
   of Wireshark, you should first upgrade to that release, as, if
   there's a bug of that sort, it might've been fixed in a release
   after the one you're running. If the hang occurs in the most
   recent release of Wireshark, the bug should be reported to the
   Wireshark developers' mailing list at
   wireshark-dev@wireshark.org.
   On UNIX-flavored OSes, please try to force Wireshark to dump
   core, by sending it a SIGABRT signal (usually signal 6) with
   the kill command, and then get a stack trace if you have a
   debugger installed. A stack trace can be obtained by using your
   debugger (gdb in this example), the Wireshark binary, and the
   resulting core file. Here's an example of how to use the gdb
   command backtrace to do so.



        $ gdb wireshark core

        (gdb) backtrace

        ..... prints the stack trace

        (gdb) quit

        $



   The core dump file may be named "wireshark.core" rather than
   "core" on some platforms (e.g., BSD systems).
   Also, if at all possible, please send a copy of the capture
   file that caused the problem. When capturing packets, Wireshark
   normally writes captured packets to a temporary file, which
   will probably be in /tmp or /var/tmp on UNIX-flavored OSes,
   \TEMP on the main system disk (normally \Documents and
   Settings\your login name \Local Settings\Temp on the main
   system disk on Windows Windows XP and Server 2003, and
   \Users\your login name\AppData\Local\Temp on the main system
   disk on Windows Vista and later, so the capture file will
   probably be there. If you are capturing on a single interface,
   it will have a name of the form,
   wireshark_<iface>_YYYYmmddHHMMSS_XXXXXX.<fmt>, where <fmt> is
   the capture file format (pcap or pcapng), and <iface> is the
   actual name of the interface you are capturing on; otherwise,
   if you are capturing on multiple interfaces, it will have a
   name of the form,
   wireshark_<N>_interfaces_YYYYmmddHHMMSS_XXXXXX.<fmt>, where <N>
   is the number of simultaneous interfaces you are capturing on.
   Please don't send a trace file greater than 1 MB when
   compressed; instead, make it available via FTP or HTTP, or say
   it's available but leave it up to a developer to ask for it. If
   the trace file contains sensitive information (e.g.,
   passwords), then please do not send it.

  7. Capturing packets on Windows

   Q 7.1: I'm running Wireshark on Windows; why does some network
   interface on my machine not show up in the list of interfaces
   in the "Interface:" field in the dialog box popped up by
   "Capture->Start", and/or why does Wireshark give me an error if
   I try to capture on that interface?

   A: If you are running Wireshark on Windows XP, or Windows
   Server 2003, and this is the first time you have run a
   WinPcap-based program (such as Wireshark, or TShark, or
   WinDump, or Analyzer, or...) since the machine was rebooted,
   you need to run that program from an account with administrator
   privileges; once you have run such a program, you will not need
   administrator privileges to run any such programs until you
   reboot.
   If you are running on Windows Windows XP or Windows Server 2003
   and have administrator privileges or a WinPcap-based program
   has been run with those privileges since the machine rebooted,
   this problem might clear up if you completely un-install
   WinPcap and then re-install it.
   If that doesn't work, then note that Wireshark relies on the
   WinPcap library, on the WinPcap device driver, and on the
   facilities that come with the OS on which it's running in order
   to do captures.
   Therefore, if the OS, the WinPcap library, or the WinPcap
   driver don't support capturing on a particular network
   interface device, Wireshark won't be able to capture on that
   device.
   WinPcap 2.3 has problems supporting PPP WAN interfaces on
   Windows NT 4.0, Windows 2000, Windows XP, and Windows Server
   2003, and, to avoid those problems, support for PPP WAN
   interfaces on those versions of Windows has been disabled in
   WinPcap 3.0. Regular dial-up lines, ISDN lines, ADSL
   connections using PPPoE or PPPoA, and various other lines such
   as T1/E1 lines are all PPP interfaces, so those interfaces
   might not show up on the list of interfaces in the "Capture
   Options" dialog on those OSes.
   On Windows 2000, Windows XP, and Windows Server 2003, but not
   Windows NT 4.0 or Windows Vista Beta 1, you should be able to
   capture on the "GenericDialupAdapter" with WinPcap 3.1. (3.1
   beta releases called it the "NdisWanAdapter"; if you're using a
   3.1 beta release, you should un-install it and install the
   final 3.1 release.) See the Wireshark Wiki item on PPP
   capturing for details.
   WinPcap prior to 3.0 does not support multiprocessor machines
   (note that machines with a single multi-threaded processor,
   such as Intel's new multi-threaded x86 processors, are
   multiprocessor machines as far as the OS and WinPcap are
   concerned), and recent 2.x versions of WinPcap refuse to
   operate if they detect that they're running on a multiprocessor
   machine, which means that they may not show any network
   interfaces. You will need to use WinPcap 3.0 to capture on a
   multiprocessor machine.
   If an interface doesn't show up in the list of interfaces in
   the "Interface:" field, and you know the name of the interface,
   try entering that name in the "Interface:" field and capturing
   on that device.
   If the attempt to capture on it succeeds, the interface is
   somehow not being reported by the mechanism Wireshark uses to
   get a list of interfaces. Try listing the interfaces with
   WinDump; see the WinDump Web site for information on using
   WinDump.
   You would run WinDump with the -D flag; if it lists the
   interface, please report this to wireshark-dev@wireshark.org
   giving full details of the problem, including

     * the operating system you're using, and the version of that
       operating system;
     * the type of network device you're using;
     * the output of WinDump.

   If WinDump does not list the interface, this is almost
   certainly a problem with one or more of:

     * the operating system you're using;
     * the device driver for the interface you're using;
     * the WinPcap library and/or the WinPcap device driver;

   so first check the WinPcap FAQ to see if your problem is
   mentioned there. If not, then see the WinPcap support page -
   check the "Submitting bugs" section.
   If you are having trouble capturing on a particular network
   interface, first try capturing on that device with WinDump; see
   the WinDump Web site for information on using WinDump.
   If you can capture on the interface with WinDump, send mail to
   wireshark-users@wireshark.org giving full details of the
   problem, including

     * the operating system you're using, and the version of that
       operating system;
     * the type of network device you're using;
     * the error message you get from Wireshark.

   If you cannot capture on the interface with WinDump, this is
   almost certainly a problem with one or more of:

     * the operating system you're using;
     * the device driver for the interface you're using;
     * the WinPcap library and/or the WinPcap device driver;

   so first check the WinPcap FAQ to see if your problem is
   mentioned there. If not, then see the WinPcap support page -
   check the "Submitting bugs" section.
   You may also want to ask the wireshark-users@wireshark.org and
   the winpcap-users@winpcap.org mailing lists to see if anybody
   happens to know about the problem and know a workaround or fix
   for the problem. (Note that you will have to subscribe to that
   list in order to be allowed to mail to it; see the WinPcap
   support page for information on the mailing list.) In your
   mail, please give full details of the problem, as described
   above, and also indicate that the problem occurs with WinDump,
   not just with Wireshark.

   Q 7.2: I'm running Wireshark on Windows; why do no network
   interfaces show up in the list of interfaces in the
   "Interface:" field in the dialog box popped up by
   "Capture->Start"?

   A: This is really the same question as a previous one; see the
   response to that question.

   Q 7.3: I'm running Wireshark on Windows; why doesn't my serial
   port/ADSL modem/ISDN modem show up in the list of interfaces in
   the "Interface:" field in the dialog box popped up by
   "Capture->Start"?

   A: Internet access on those devices is often done with the
   Point-to-Point (PPP) protocol; WinPcap 2.3 has problems
   supporting PPP WAN interfaces on Windows NT 4.0, Windows 2000,
   Windows XP, and Windows Server 2003, and, to avoid those
   problems, support for PPP WAN interfaces on those versions of
   Windows has been disabled in WinPcap 3.0.
   On Windows 2000, Windows XP, and Windows Server 2003, but not
   Windows NT 4.0 or Windows Vista Beta 1, you should be able to
   capture on the "GenericDialupAdapter" with WinPcap 3.1. (3.1
   beta releases called it the "NdisWanAdapter"; if you're using a
   3.1 beta release, you should un-install it and install the
   final 3.1 release.) See the Wireshark Wiki item on PPP
   capturing for details.

   Q 7.4: I'm running Wireshark on Windows NT 4.0/Windows
   2000/Windows XP/Windows Server 2003; my machine has a PPP
   (dial-up POTS, ISDN, etc.) interface, and it shows up in the
   "Interface" item in the "Capture Options" dialog box. Why can
   no packets be sent on or received from that network while I'm
   trying to capture traffic on that interface?

   A: Some versions of WinPcap have problems with PPP WAN
   interfaces on Windows NT 4.0, Windows 2000, Windows XP, and
   Windows Server 2003; one symptom that may be seen is that
   attempts to capture in promiscuous mode on the interface cause
   the interface to be incapable of sending or receiving packets.
   You can disable promiscuous mode using the -p command-line flag
   or the item in the "Capture Preferences" dialog box, but this
   may mean that outgoing packets, or incoming packets, won't be
   seen in the capture.
   On Windows 2000, Windows XP, and Windows Server 2003, but not
   Windows NT 4.0 or Windows Vista Beta 1, you should be able to
   capture on the "GenericDialupAdapter" with WinPcap 3.1. (3.1
   beta releases called it the "NdisWanAdapter"; if you're using a
   3.1 beta release, you should un-install it and install the
   final 3.1 release.) See the Wireshark Wiki item on PPP
   capturing for details.

   Q 7.5: I'm running Wireshark on Windows; why am I not seeing
   any traffic being sent by the machine running Wireshark?

   A: If you are running some form of VPN client software, it
   might be causing this problem; people have seen this problem
   when they have Check Point's VPN software installed on their
   machine. If that's the cause of the problem, you will have to
   remove the VPN software in order to have Wireshark (or any
   other application using WinPcap) see outgoing packets;
   unfortunately, neither we nor the WinPcap developers know any
   way to make WinPcap and the VPN software work well together.
   Also, some drivers for Windows (especially some wireless
   network interface drivers) apparently do not, when running in
   promiscuous mode, arrange that outgoing packets are delivered
   to the software that requested that the interface run
   promiscuously; try turning promiscuous mode off.

   Q 7.6: When I capture on Windows in promiscuous mode, I can see
   packets other than those sent to or from my machine; however,
   those packets show up with a "Short Frame" indication, unlike
   packets to or from my machine. What should I do to arrange that
   I see those packets in their entirety?

   A: In at least some cases, this appears to be the result of
   PGPnet running on the network interface on which you're
   capturing; turn it off on that interface.

   Q 7.7: I'm trying to capture 802.11 traffic on Windows; why am
   I not seeing any packets?

   A: At least some 802.11 card drivers on Windows appear not to
   see any packets if they're running in promiscuous mode. Try
   turning promiscuous mode off; you'll only be able to see
   packets sent by and received by your machine, not third-party
   traffic, and it'll look like Ethernet traffic and won't include
   any management or control frames, but that's a limitation of
   the card drivers.
   See the archived MicroLogix's list of cards supported with
   WinPcap for information on support of various adapters and
   drivers with WinPcap.

   Q 7.8: I'm trying to capture 802.11 traffic on Windows; why am
   I seeing packets received by the machine on which I'm capturing
   traffic, but not packets sent by that machine?

   A: This appears to be another problem with promiscuous mode;
   try turning it off.

   Q 7.9: I'm trying to capture Ethernet VLAN traffic on Windows,
   and I'm capturing on a "raw" Ethernet device rather than a
   "VLAN interface", so that I can see the VLAN headers; why am I
   seeing packets received by the machine on which I'm capturing
   traffic, but not packets sent by that machine?

   A: The way the Windows networking code works probably means
   that packets are sent on a "VLAN interface" rather than the
   "raw" device, so packets sent by the machine will only be seen
   when you capture on the "VLAN interface". If so, you will be
   unable to see outgoing packets when capturing on the "raw"
   device, so you are stuck with a choice between seeing VLAN
   headers and seeing outgoing packets.

  8. Capturing packets on UN*Xes

   Q 8.1: I'm running Wireshark on a UNIX-flavored OS; why does
   some network interface on my machine not show up in the list of
   interfaces in the "Interface:" field in the dialog box popped
   up by "Capture->Start", and/or why does Wireshark give me an
   error if I try to capture on that interface?

   A: You may need to run Wireshark from an account with
   sufficient privileges to capture packets, such as the
   super-user account, or may need to give your account sufficient
   privileges to capture packets. Only those interfaces that
   Wireshark can open for capturing show up in that list; if you
   don't have sufficient privileges to capture on any interfaces,
   no interfaces will show up in the list. See the Wireshark Wiki
   item on capture privileges for details on how to give a
   particular account or account group capture privileges on
   platforms where that can be done.
   If you are running Wireshark from an account with sufficient
   privileges, then note that Wireshark relies on the libpcap
   library, and on the facilities that come with the OS on which
   it's running in order to do captures. On some OSes, those
   facilities aren't present by default; see the Wireshark Wiki
   item on adding capture support for details.
   And, even if you're running with an account that has sufficient
   privileges to capture, and capture support is present in your
   OS, if the OS or the libpcap library don't support capturing on
   a particular network interface device or particular types of
   devices, Wireshark won't be able to capture on that device.
   On Solaris, note that libpcap 0.6.2 and earlier didn't support
   Token Ring interfaces; the current version, 0.7.2, does support
   Token Ring, and the current version of Wireshark works with
   libpcap 0.7.2 and later.
   If an interface doesn't show up in the list of interfaces in
   the "Interface:" field, and you know the name of the interface,
   try entering that name in the "Interface:" field and capturing
   on that device.
   If the attempt to capture on it succeeds, the interface is
   somehow not being reported by the mechanism Wireshark uses to
   get a list of interfaces; please report this to
   wireshark-dev@wireshark.org giving full details of the problem,
   including

     * the operating system you're using, and the version of that
       operating system (for Linux, give both the version number
       of the kernel and the name and version number of the
       distribution you're using);
     * the type of network device you're using.

   If you are having trouble capturing on a particular network
   interface, and you've made sure that (on platforms that require
   it) you've arranged that packet capture support is present, as
   per the above, first try capturing on that device with tcpdump.
   If you can capture on the interface with tcpdump, send mail to
   wireshark-users@wireshark.org giving full details of the
   problem, including

     * the operating system you're using, and the version of that
       operating system (for Linux, give both the version number
       of the kernel and the name and version number of the
       distribution you're using);
     * the type of network device you're using;
     * the error message you get from Wireshark.

   If you cannot capture on the interface with tcpdump, this is
   almost certainly a problem with one or more of:

     * the operating system you're using;
     * the device driver for the interface you're using;
     * the libpcap library;

   so you should report the problem to the company or organization
   that produces the OS (in the case of a Linux distribution,
   report the problem to whoever produces the distribution).
   You may also want to ask the wireshark-users@wireshark.org and
   the tcpdump-workers@lists.tcpdump.org mailing lists to see if
   anybody happens to know about the problem and know a workaround
   or fix for the problem. In your mail, please give full details
   of the problem, as described above, and also indicate that the
   problem occurs with tcpdump not just with Wireshark.

   Q 8.2: I'm running Wireshark on a UNIX-flavored OS; why do no
   network interfaces show up in the list of interfaces in the
   "Interface:" field in the dialog box popped up by
   "Capture->Start"?

   A: This is really the same question as the previous one; see
   the response to that question.

   Q 8.3: I'm capturing packets on Linux; why do the time stamps
   have only 100ms resolution, rather than 1us resolution?

   A: Wireshark gets time stamps from libpcap/WinPcap, and
   libpcap/WinPcap get them from the OS kernel, so Wireshark - and
   any other program using libpcap, such as tcpdump - is at the
   mercy of the time stamping code in the OS for time stamps.
   At least on x86-based machines, Linux can get high-resolution
   time stamps on newer processors with the Time Stamp Counter
   (TSC) register; for example, Intel x86 processors, starting
   with the Pentium Pro, and including all x86 processors since
   then, have had a TSC, and other vendors probably added the TSC
   at some point to their families of x86 processors. The Linux
   kernel must be configured with the CONFIG_X86_TSC option
   enabled in order to use the TSC. Make sure this option is
   enabled in your kernel.
   In addition, some Linux distributions may have bugs in their
   versions of the kernel that cause packets not to be given
   high-resolution time stamps even if the TSC is enabled. See,
   for example, bug 61111 for Red Hat Linux 7.2. If your
   distribution has a bug such as this, you may have to run a
   standard kernel from kernel.org in order to get high-resolution
   time stamps.

  9. Capturing packets on wireless LANs

   Q 9.1: How can I capture raw 802.11 frames, including non-data
   (management, beacon) frames?

   A: That depends on the operating system on which you're
   running, and on the 802.11 interface on which you're capturing.
   This would probably require that you capture in promiscuous
   mode or in the mode called "monitor mode" or "RFMON mode". On
   some platforms, or with some cards, this might require that you
   capture in monitor mode - promiscuous mode might not be
   sufficient. If you want to capture traffic on networks other
   than the one with which you're associated, you will have to
   capture in monitor mode.
   Not all operating systems support capturing non-data packets
   and, even on operating systems that do support it, not all
   drivers, and thus not all interfaces, support it. Even on those
   that do, monitor mode might not be supported by the operating
   system or by the drivers for all interfaces.
   NOTE: an interface running in monitor mode will, on most if not
   all platforms, not be able to act as a regular network
   interface; putting it into monitor mode will, in effect, take
   your machine off of whatever network it's on as long as the
   interface is in monitor mode, allowing it only to passively
   capture packets.
   This means that you should disable name resolution when
   capturing in monitor mode; otherwise, when Wireshark (or
   TShark, or tcpdump) tries to display IP addresses as host
   names, it will probably block for a long time trying to resolve
   the name because it will not be able to communicate with any
   DNS or NIS servers.
   See the Wireshark Wiki item on 802.11 capturing for details.

   Q 9.2: How do I capture on an 802.11 device in monitor mode?

   A: Whether you will be able to capture in monitor mode depends
   on the operating system, adapter, and driver you're using. See
   the previous question for information on monitor mode,
   including a link to the Wireshark Wiki page that gives details
   on 802.11 capturing.

  10. Viewing traffic

   Q 10.1: Why am I seeing lots of packets with incorrect TCP
   checksums?

   A: If the packets that have incorrect TCP checksums are all
   being sent by the machine on which Wireshark is running, this
   is probably because the network interface on which you're
   capturing does TCP checksum offloading. That means that the TCP
   checksum is added to the packet by the network interface, not
   by the OS's TCP/IP stack; when capturing on an interface,
   packets being sent by the host on which you're capturing are
   directly handed to the capture interface by the OS, which means
   that they are handed to the capture interface without a TCP
   checksum being added to them.
   The only way to prevent this from happening would be to disable
   TCP checksum offloading, but

    1. that might not even be possible on some OSes;
    2. that could reduce networking performance significantly.

   However, you can disable the check that Wireshark does of the
   TCP checksum, so that it won't report any packets as having TCP
   checksum errors, and so that it won't refuse to do TCP
   reassembly due to a packet having an incorrect TCP checksum.
   That can be set as an Wireshark preference by selecting
   "Preferences" from the "Edit" menu, opening up the "Protocols"
   list in the left-hand pane of the "Preferences" dialog box,
   selecting "TCP", from that list, turning off the "Check the
   validity of the TCP checksum when possible" option, clicking
   "Save" if you want to save that setting in your preference
   file, and clicking "OK".
   It can also be set on the Wireshark or TShark command line with
   a -o tcp.check_checksum:false command-line flag, or manually
   set in your preferences file by adding a
   tcp.check_checksum:false line.

   Q 10.2: I've just installed Wireshark, and the traffic on my
   local LAN is boring. Where can I find more interesting
   captures?

   A: We have a collection of strange and exotic sample capture
   files at https://wiki.wireshark.org/SampleCaptures

   Q 10.3: Why doesn't Wireshark correctly identify RTP packets?
   It shows them only as UDP.

   A: Wireshark can identify a UDP datagram as containing a packet
   of a particular protocol running atop UDP only if

    1. The protocol in question has a particular standard port
       number, and the UDP source or destination port number is
       that port
    2. Packets of that protocol can be identified by looking for a
       "signature" of some type in the packet - i.e., some data
       that, if Wireshark finds it in some particular part of a
       packet, means that the packet is almost certainly a packet
       of that type.
    3. Some other traffic earlier in the capture indicated that,
       for example, UDP traffic between two particular addresses
       and ports will be RTP traffic.

   RTP doesn't have a standard port number, so 1) doesn't work; it
   doesn't, as far as I know, have any "signature", so 2) doesn't
   work.
   That leaves 3). If there's RTSP traffic that sets up an RTP
   session, then, at least in some cases, the RTSP dissector will
   set things up so that subsequent RTP traffic will be
   identified. Currently, that's the only place we do that; there
   may be other places.
   However, there will always be places where Wireshark is simply
   incapable of deducing that a given UDP flow is RTP; a mechanism
   would be needed to allow the user to specify that a given
   conversation should be treated as RTP. As of Wireshark 0.8.16,
   such a mechanism exists; if you select a UDP or TCP packet, the
   right mouse button menu will have a "Decode As..." menu item,
   which will pop up a dialog box letting you specify that the
   source port, the destination port, or both the source and
   destination ports of the packet should be dissected as some
   particular protocol.

   Q 10.4: Why doesn't Wireshark show Yahoo Messenger packets in
   captures that contain Yahoo Messenger traffic?

   A: Wireshark only recognizes as Yahoo Messenger traffic packets
   to or from TCP port 3050 that begin with "YPNS", "YHOO", or
   "YMSG". TCP segments that start with the middle of a Yahoo
   Messenger packet that takes more than one TCP segment will not
   be recognized as Yahoo Messenger packets (even if the TCP
   segment also contains the beginning of another Yahoo Messenger
   packet).

  11. Filtering traffic

   Q 11.1: I saved a filter and tried to use its name to filter
   the display; why do I get an "Unexpected end of filter string"
   error?

   A: You cannot use the name of a saved display filter as a
   filter. To filter the display, you can enter a display filter
   expression - not the name of a saved display filter - in the
   "Filter:" box at the bottom of the display, and type the
   <Enter> key or press the "Apply" button (that does not require
   you to have a saved filter), or, if you want to use a saved
   filter, you can press the "Filter:" button, select the filter
   in the dialog box that pops up, and press the "OK" button.

   Q 11.2: How can I search for, or filter, packets that have a
   particular string anywhere in them?

   A: If you want to do this when capturing, you can't. That's a
   feature that would be hard to implement in capture filters
   without changes to the capture filter code, which, on many
   platforms, is in the OS kernel and, on other platforms, is in
   the libpcap library.
   After capture, you can search for text by selecting Edit→Find
   Packet... and making sure String is selected. Alternately, you
   can use the "contains" display filter operator or "matches"
   operator if it's supported on your system.

   Q 11.3: How do I filter a capture to see traffic for virus XXX?

   A: For some viruses/worms there might be a capture filter to
   recognize the virus traffic. Check the CaptureFilters page on
   the Wireshark Wiki to see if anybody's added such a filter.
   Note that Wireshark was not designed to be an intrusion
   detection system; you might be able to use it as an IDS, but in
   most cases software designed to be an IDS, such as Snort or
   Prelude, will probably work better.

