To try samba 2.0.7 for OS/2
==============================================================================
First remove netbios over ip from your mpts and reboot
(because it starts programs using ports needed by samba)
==============================================================================
Launch smbd -D   (-D start smbd as Daemon)
use smbclient -Lxxxx  where xxx is your hostname present in you hosts file
                      or resolved by your dns
                      to see if it work host xxxx it must give you a ip address
by default the user used by samba is the user define in the env var user
so SET USER=f731 in config.sys
and
smbclient -LTP390X            list all the resource of the pc TP390X logon
                              with f731 (it's your net share comment in LS OS/2)
smbclient -LTP390X -U f947    same as above but we force the user to be f947

smblclient //TP390X/d$        get the d: drive of tp390X we are connected with f731
smbclinet //TP390X/d$ -U f731 same as above but with f731
